LISA MODEL DESCRIPTION FORMAT 6.1
=================================
Design:   COMVDD MULTIMATHS POTS MODEL
Doc. no.: 002
Revision: 002
Author:   SIMEON.DAVID.WEBBER.MCA
Created:  10/09/05
Modified: 17/07/06

*PROPERTIES,119  
ANTILOGTAPER1=<ANTILOGTAPER1>
ANTILOGTAPER2=<ANTILOGTAPER2>
ANTILOGTAPER3=<ANTILOGTAPER3>
ANTILOGTAPER4=<ANTILOGTAPER4>
ANTILOGTAPER5=<ANTILOGTAPER5>
ANTILOGTAPER6=<ANTILOGTAPER6>
ANTILOGTAPER7=<ANTILOGTAPER7>
ANTILOGTAPER8=<ANTILOGTAPER8>
ANTILOGTAPER9=<ANTILOGTAPER9>
ANTILOGTAPER10=<ANTILOGTAPER10>
ANTILOGTAPER11=<ANTILOGTAPER11>
ANTILOGTAPER12=<ANTILOGTAPER12>
ANTILOGTAPER13=<ANTILOGTAPER13>
ANTILOGTAPER14=<ANTILOGTAPER14>
ANTILOGTAPER15=<ANTILOGTAPER15>
ANTILOGTAPER16=<ANTILOGTAPER16>
APUDFREQ=<APUDFREQ>
BTE=<BTE>
BTNOFFRES=<BTNOFFRES>
BTNONRES=<BTNONRES>
BTNSWTIME=<BTNSWTIME>
BTSWITCH=<BTSWITCH>
BUTTONS=<BUTTONS>
CRM=<CRM>
DEC=<DEC>
DECADE=<DECADE>
DM=<DM>
DS=<DS>
ENSAVED=<ENSAVED>
GCPP1=<GCPP1>
GCPP2=<GCPP2>
GCPP3=<GCPP3>
GCPP4=<GCPP4>
GCPP5=<GCPP5>
GCPP6=<GCPP6>
GCPP7=<GCPP7>
GCPP8=<GCPP8>
GCPP9=<GCPP9>
GCPP10=<GCPP10>
GCPP11=<GCPP11>
GCPP12=<GCPP12>
GCPP13=<GCPP13>
GCPP14=<GCPP14>
GCPP15=<GCPP15>
GCPP16=<GCPP16>
GR1=<GR1>
GR2=<GR2>
GR3=<GR3>
GR4=<GR4>
GR5=<GR5>
GR6=<GR6>
GR7=<GR7>
GR8=<GR8>
GR9=<GR9>
GR10=<GR10>
GR11=<GR11>
GR12=<GR12>
GR13=<GR13>
GR14=<GR14>
GR15=<GR15>
GR16=<GR16>
HIDEOA=<HIDEOA>
INITBTNS=<INITBTNS>
INITSW=<INITSW>
LOGTAPER1=<LOGTAPER1>
LOGTAPER2=<LOGTAPER2>
LOGTAPER3=<LOGTAPER3>
LOGTAPER4=<LOGTAPER4>
LOGTAPER5=<LOGTAPER5>
LOGTAPER6=<LOGTAPER6>
LOGTAPER7=<LOGTAPER7>
LOGTAPER8=<LOGTAPER8>
LOGTAPER9=<LOGTAPER9>
LOGTAPER10=<LOGTAPER10>
LOGTAPER11=<LOGTAPER11>
LOGTAPER12=<LOGTAPER12>
LOGTAPER13=<LOGTAPER13>
LOGTAPER14=<LOGTAPER14>
LOGTAPER15=<LOGTAPER15>
LOGTAPER16=<LOGTAPER16>
POTVAL1=<POTVAL1>
POTVAL2=<POTVAL2>
POTVAL3=<POTVAL3>
POTVAL4=<POTVAL4>
POTVAL5=<POTVAL5>
POTVAL6=<POTVAL6>
POTVAL7=<POTVAL7>
POTVAL8=<POTVAL8>
POTVAL9=<POTVAL9>
POTVAL10=<POTVAL10>
POTVAL11=<POTVAL11>
POTVAL12=<POTVAL12>
POTVAL13=<POTVAL13>
POTVAL14=<POTVAL14>
POTVAL15=<POTVAL15>
POTVAL16=<POTVAL16>
PRERETRY=<PRERETRY>
PSDELAY=<PSDELAY>
PTM=<PTM>
PUVIEW=<PUVIEW>
RSPREAD=100T
SDSSW=<SDSSW>
SHMEM=<SHMEM>
SIMRETRY=<SIMRETRY>
SLIDERS=<SLIDERS>
SPRINGEN=<SPRINGEN>
SSDELAY=<SSDELAY>
SSPU=<SSPU>
STSWITCH=<STSWITCH>
SWITCHES=<SWITCHES>
SWOFFRES=<SWOFFRES>
SWONRES=<SWONRES>
SWSWTIME=<SWSWTIME>
VD_BAUDRATE=<VD_BAUDRATE>
VD_DATABITS=<VD_DATABITS>
VD_PARITY=<VD_PARITY>
VD_PORT=<VD_PORT>
VD_STOPBITS=<VD_STOPBITS>
VDD=<VDD>

*MAPPINGS,16,APOTS
1 : XPOTS = 0,     ptCONV=1u , tsbCONV=2u
2 : XPOTS = 1,     ptCONV=1u , tsbCONV=2u
3 : XPOTS = 2,     ptCONV=1u , tsbCONV=2u
4 : XPOTS = 3,     ptCONV=1u , tsbCONV=2u
5 : XPOTS = 4,     ptCONV=1u , tsbCONV=2u
6 : XPOTS = 5,     ptCONV=1u , tsbCONV=2u
7 : XPOTS = 6,     ptCONV=1u , tsbCONV=2u
8 : XPOTS = 7,     ptCONV=1u , tsbCONV=2u
9 : XPOTS = 8,     ptCONV=1u , tsbCONV=2u
10 : XPOTS = 9,     ptCONV=1u , tsbCONV=2u
11 : XPOTS = 10,   ptCONV=1u , tsbCONV=2u
12 : XPOTS = 11,   ptCONV=1u , tsbCONV=2u
13 : XPOTS = 12,   ptCONV=1u , tsbCONV=2u
14 : XPOTS = 13,   ptCONV=1u , tsbCONV=2u
15 : XPOTS = 14,   ptCONV=1u , tsbCONV=2u
16 : XPOTS = 15,   ptCONV=1u , tsbCONV=2u

*MAPPINGS,14,STEP1
10 : AW_1VOLTS = 10,     BW_1VOLTS = 10,     AVS1VOLTS = 10,     REFV1 = 10
16 : AW_1VOLTS =  16,      BW_1VOLTS = 16,       AVS1VOLTS = 16,       REFV1 = 16
32 : AW_1VOLTS =  32,      BW_1VOLTS = 32,       AVS1VOLTS = 32,       REFV1 = 32
64 : AW_1VOLTS =  64,      BW_1VOLTS = 64,       AVS1VOLTS = 64,       REFV1 = 64
100 : AW_1VOLTS = 100,     BW_1VOLTS = 100,     AVS1VOLTS = 100,     REFV1 = 100
128 : AW_1VOLTS =  128,      BW_1VOLTS = 128,       AVS1VOLTS = 128,       REFV1 = 128
256 : AW_1VOLTS =  256,      BW_1VOLTS = 256,       AVS1VOLTS = 256,       REFV1 = 256
512 : AW_1VOLTS =  512,      BW_1VOLTS = 512,       AVS1VOLTS = 512,       REFV1 = 512
655.35 : AW_1VOLTS =  655.35, BW_1VOLTS = 655.35,  AVS1VOLTS = 655.35,  REFV1 = 655.35
1000 : AW_1VOLTS = 1000,     BW_1VOLTS = 1000,     AVS1VOLTS = 1000,     REFV1 = 1000
1024 : AW_1VOLTS =  1024,    BW_1VOLTS = 1024,     AVS1VOLTS = 1024,     REFV1 = 1024
10000 : AW_1VOLTS = 10000,     BW_1VOLTS = 10000,     AVS1VOLTS = 10000,     REFV1 = 10000
32768 : AW_1VOLTS =  32768,  BW_1VOLTS = 32768,   AVS1VOLTS = 32768,   REFV1 = 32768
65535 : AW_1VOLTS =  65535,  BW_1VOLTS = 65535,   AVS1VOLTS = 65535,   REFV1 = 65535

*MAPPINGS,14,STEP2
10 : AW_2VOLTS = 10,     BW_2VOLTS = 10,     AVS2VOLTS = 10,     REFV2 = 10
16 : AW_2VOLTS =  16,      BW_2VOLTS = 16,       AVS2VOLTS = 16,       REFV2 = 16
32 : AW_2VOLTS =  32,      BW_2VOLTS = 32,       AVS2VOLTS = 32,       REFV2 = 32
64 : AW_2VOLTS =  64,      BW_2VOLTS = 64,       AVS2VOLTS = 64,       REFV2 = 64
100 : AW_2VOLTS = 100,     BW_2VOLTS = 100,     AVS2VOLTS = 100,     REFV2 = 100
128 : AW_2VOLTS =  128,      BW_2VOLTS = 128,       AVS2VOLTS = 128,       REFV2 = 128
256 : AW_2VOLTS =  256,      BW_2VOLTS = 256,       AVS2VOLTS = 256,       REFV2 = 256
512 : AW_2VOLTS =  512,      BW_2VOLTS = 512,       AVS2VOLTS = 512,       REFV2 = 512
655.35 : AW_2VOLTS =  655.35, BW_2VOLTS = 655.35,  AVS2VOLTS = 655.35,  REFV2 = 655.35
1000 : AW_2VOLTS = 1000,     BW_2VOLTS = 1000,     AVS2VOLTS = 1000,     REFV2 = 1000
1024 : AW_2VOLTS =  1024,    BW_2VOLTS = 1024,     AVS2VOLTS = 1024,     REFV2 = 1024
10000 : AW_2VOLTS = 10000,     BW_2VOLTS = 10000,     AVS2VOLTS = 10000,     REFV2 = 10000
32768 : AW_2VOLTS =  32768,  BW_2VOLTS = 32768,   AVS2VOLTS = 32768,   REFV2 = 32768
65535 : AW_2VOLTS =  65535,  BW_2VOLTS = 65535,   AVS2VOLTS = 65535,   REFV2 = 65535

*MAPPINGS,14,STEP3
10 : AW_3VOLTS = 10,     BW_3VOLTS = 10,     AVS3VOLTS = 10,     REFV3 = 10
16 : AW_3VOLTS =  16,      BW_3VOLTS = 16,       AVS3VOLTS = 16,       REFV3 = 16
32 : AW_3VOLTS =  32,      BW_3VOLTS = 32,       AVS3VOLTS = 32,       REFV3 = 32
64 : AW_3VOLTS =  64,      BW_3VOLTS = 64,       AVS3VOLTS = 64,       REFV3 = 64
100 : AW_3VOLTS = 100,     BW_3VOLTS = 100,     AVS3VOLTS = 100,     REFV3 = 100
128 : AW_3VOLTS =  128,      BW_3VOLTS = 128,       AVS3VOLTS = 128,       REFV3 = 128
256 : AW_3VOLTS =  256,      BW_3VOLTS = 256,       AVS3VOLTS = 256,       REFV3 = 256
512 : AW_3VOLTS =  512,      BW_3VOLTS = 512,       AVS3VOLTS = 512,       REFV3 = 512
655.35 : AW_3VOLTS =  655.35, BW_3VOLTS = 655.35,  AVS3VOLTS = 655.35,  REFV3 = 655.35
1000 : AW_3VOLTS = 1000,     BW_3VOLTS = 1000,     AVS3VOLTS = 1000,     REFV3 = 1000
1024 : AW_3VOLTS =  1024,    BW_3VOLTS = 1024,     AVS3VOLTS = 1024,     REFV3 = 1024
10000 : AW_3VOLTS = 10000,     BW_3VOLTS = 10000,     AVS3VOLTS = 10000,     REFV3 = 10000
32768 : AW_3VOLTS =  32768,  BW_3VOLTS = 32768,   AVS3VOLTS = 32768,   REFV3 = 32768
65535 : AW_3VOLTS =  65535,  BW_3VOLTS = 65535,   AVS3VOLTS = 65535,   REFV3 = 65535

*MAPPINGS,14,STEP4
10 : AW_4VOLTS = 10,     BW_4VOLTS = 10,     AVS4VOLTS = 10,     REFV4 = 10
16 : AW_4VOLTS =  16,      BW_4VOLTS = 16,       AVS4VOLTS = 16,       REFV4 = 16
32 : AW_4VOLTS =  32,      BW_4VOLTS = 32,       AVS4VOLTS = 32,       REFV4 = 32
64 : AW_4VOLTS =  64,      BW_4VOLTS = 64,       AVS4VOLTS = 64,       REFV4 = 64
100 : AW_4VOLTS = 100,     BW_4VOLTS = 100,     AVS4VOLTS = 100,     REFV4 = 100
128 : AW_4VOLTS =  128,      BW_4VOLTS = 128,       AVS4VOLTS = 128,       REFV4 = 128
256 : AW_4VOLTS =  256,      BW_4VOLTS = 256,       AVS4VOLTS = 256,       REFV4 = 256
512 : AW_4VOLTS =  512,      BW_4VOLTS = 512,       AVS4VOLTS = 512,       REFV4 = 512
655.35 : AW_4VOLTS =  655.35, BW_4VOLTS = 655.35,  AVS4VOLTS = 655.35,  REFV4 = 655.35
1000 : AW_4VOLTS = 1000,     BW_4VOLTS = 1000,     AVS4VOLTS = 1000,     REFV4 = 1000
1024 : AW_4VOLTS =  1024,    BW_4VOLTS = 1024,     AVS4VOLTS = 1024,     REFV4 = 1024
10000 : AW_4VOLTS = 10000,     BW_4VOLTS = 10000,     AVS4VOLTS = 10000,     REFV4 = 10000
32768 : AW_4VOLTS =  32768,  BW_4VOLTS = 32768,   AVS4VOLTS = 32768,   REFV4 = 32768
65535 : AW_4VOLTS =  65535,  BW_4VOLTS = 65535,   AVS4VOLTS = 65535,   REFV4 = 65535

*MAPPINGS,14,STEP5
10 : AW_5VOLTS = 10,     BW_5VOLTS = 10,     AVS5VOLTS = 10,     REFV5 = 10
16 : AW_5VOLTS =  16,      BW_5VOLTS = 16,       AVS5VOLTS = 16,       REFV5 = 16
32 : AW_5VOLTS =  32,      BW_5VOLTS = 32,       AVS5VOLTS = 32,       REFV5 = 32
64 : AW_5VOLTS =  64,      BW_5VOLTS = 64,       AVS5VOLTS = 64,       REFV5 = 64
100 : AW_5VOLTS = 100,     BW_5VOLTS = 100,     AVS5VOLTS = 100,     REFV5 = 100
128 : AW_5VOLTS =  128,      BW_5VOLTS = 128,       AVS5VOLTS = 128,       REFV5 = 128
256 : AW_5VOLTS =  256,      BW_5VOLTS = 256,       AVS5VOLTS = 256,       REFV5 = 256
512 : AW_5VOLTS =  512,      BW_5VOLTS = 512,       AVS5VOLTS = 512,       REFV5 = 512
655.35 : AW_5VOLTS =  655.35, BW_5VOLTS = 655.35,  AVS5VOLTS = 655.35,  REFV5 = 655.35
1000 : AW_5VOLTS = 1000,     BW_5VOLTS = 1000,     AVS5VOLTS = 1000,     REFV5 = 1000
1024 : AW_5VOLTS =  1024,    BW_5VOLTS = 1024,     AVS5VOLTS = 1024,     REFV5 = 1024
10000 : AW_5VOLTS = 10000,     BW_5VOLTS = 10000,     AVS5VOLTS = 10000,     REFV5 = 10000
32768 : AW_5VOLTS =  32768,  BW_5VOLTS = 32768,   AVS5VOLTS = 32768,   REFV5 = 32768
65535 : AW_5VOLTS =  65535,  BW_5VOLTS = 65535,   AVS5VOLTS = 65535,   REFV5 = 65535

*MAPPINGS,14,STEP6
10 : AW_6VOLTS = 10,     BW_6VOLTS = 10,     AVS6VOLTS = 10,     REFV6 = 10
16 : AW_6VOLTS =  16,      BW_6VOLTS = 16,       AVS6VOLTS = 16,       REFV6 = 16
32 : AW_6VOLTS =  32,      BW_6VOLTS = 32,       AVS6VOLTS = 32,       REFV6 = 32
64 : AW_6VOLTS =  64,      BW_6VOLTS = 64,       AVS6VOLTS = 64,       REFV6 = 64
100 : AW_6VOLTS = 100,     BW_6VOLTS = 100,     AVS6VOLTS = 100,     REFV6 = 100
128 : AW_6VOLTS =  128,      BW_6VOLTS = 128,       AVS6VOLTS = 128,       REFV6 = 128
256 : AW_6VOLTS =  256,      BW_6VOLTS = 256,       AVS6VOLTS = 256,       REFV6 = 256
512 : AW_6VOLTS =  512,      BW_6VOLTS = 512,       AVS6VOLTS = 512,       REFV6 = 512
655.35 : AW_6VOLTS =  655.35, BW_6VOLTS = 655.35,  AVS6VOLTS = 655.35,  REFV6 = 655.35
1000 : AW_6VOLTS = 1000,     BW_6VOLTS = 1000,     AVS6VOLTS = 1000,     REFV6 = 1000
1024 : AW_6VOLTS =  1024,    BW_6VOLTS = 1024,     AVS6VOLTS = 1024,     REFV6 = 1024
10000 : AW_6VOLTS = 10000,     BW_6VOLTS = 10000,     AVS6VOLTS = 10000,     REFV6 = 10000
32768 : AW_6VOLTS =  32768,  BW_6VOLTS = 32768,   AVS6VOLTS = 32768,   REFV6 = 32768
65535 : AW_6VOLTS =  65535,  BW_6VOLTS = 65535,   AVS6VOLTS = 65535,   REFV6 = 65535

*MAPPINGS,14,STEP7
10 : AW_7VOLTS = 10,     BW_7VOLTS = 10,     AVS7VOLTS = 10,     REFV7 = 10
16 : AW_7VOLTS =  16,      BW_7VOLTS = 16,       AVS7VOLTS = 16,       REFV7 = 16
32 : AW_7VOLTS =  32,      BW_7VOLTS = 32,       AVS7VOLTS = 32,       REFV7 = 32
64 : AW_7VOLTS =  64,      BW_7VOLTS = 64,       AVS7VOLTS = 64,       REFV7 = 64
100 : AW_7VOLTS = 100,     BW_7VOLTS = 100,     AVS7VOLTS = 100,     REFV7 = 100
128 : AW_7VOLTS =  128,      BW_7VOLTS = 128,       AVS7VOLTS = 128,       REFV7 = 128
256 : AW_7VOLTS =  256,      BW_7VOLTS = 256,       AVS7VOLTS = 256,       REFV7 = 256
512 : AW_7VOLTS =  512,      BW_7VOLTS = 512,       AVS7VOLTS = 512,       REFV7 = 512
655.35 : AW_7VOLTS =  655.35, BW_7VOLTS = 655.35,  AVS7VOLTS = 655.35,  REFV7 = 655.35
1000 : AW_7VOLTS = 1000,     BW_7VOLTS = 1000,     AVS7VOLTS = 1000,     REFV7 = 1000
1024 : AW_7VOLTS =  1024,    BW_7VOLTS = 1024,     AVS7VOLTS = 1024,     REFV7 = 1024
10000 : AW_7VOLTS = 10000,     BW_7VOLTS = 10000,     AVS7VOLTS = 10000,     REFV7 = 10000
32768 : AW_7VOLTS =  32768,  BW_7VOLTS = 32768,   AVS7VOLTS = 32768,   REFV7 = 32768
65535 : AW_7VOLTS =  65535,  BW_7VOLTS = 65535,   AVS7VOLTS = 65535,   REFV7 = 65535

*MAPPINGS,14,STEP8
10 : AW_8VOLTS = 10,     BW_8VOLTS = 10,     AVS8VOLTS = 10,     REFV8 = 10
16 : AW_8VOLTS =  16,      BW_8VOLTS = 16,       AVS8VOLTS = 16,       REFV8 = 16
32 : AW_8VOLTS =  32,      BW_8VOLTS = 32,       AVS8VOLTS = 32,       REFV8 = 32
64 : AW_8VOLTS =  64,      BW_8VOLTS = 64,       AVS8VOLTS = 64,       REFV8 = 64
100 : AW_8VOLTS = 100,     BW_8VOLTS = 100,     AVS8VOLTS = 100,     REFV8 = 100
128 : AW_8VOLTS =  128,      BW_8VOLTS = 128,       AVS8VOLTS = 128,       REFV8 = 128
256 : AW_8VOLTS =  256,      BW_8VOLTS = 256,       AVS8VOLTS = 256,       REFV8 = 256
512 : AW_8VOLTS =  512,      BW_8VOLTS = 512,       AVS8VOLTS = 512,       REFV8 = 512
655.35 : AW_8VOLTS =  655.35, BW_8VOLTS = 655.35,  AVS8VOLTS = 655.35,  REFV8 = 655.35
1000 : AW_8VOLTS = 1000,     BW_8VOLTS = 1000,     AVS8VOLTS = 1000,     REFV8 = 1000
1024 : AW_8VOLTS =  1024,    BW_8VOLTS = 1024,     AVS8VOLTS = 1024,     REFV8 = 1024
10000 : AW_8VOLTS = 10000,     BW_8VOLTS = 10000,     AVS8VOLTS = 10000,     REFV8 = 10000
32768 : AW_8VOLTS =  32768,  BW_8VOLTS = 32768,   AVS8VOLTS = 32768,   REFV8 = 32768
65535 : AW_8VOLTS =  65535,  BW_8VOLTS = 65535,   AVS8VOLTS = 65535,   REFV8 = 65535

*MAPPINGS,14,STEP9
10 : AW_9VOLTS = 10,     BW_9VOLTS = 10,     AVS9VOLTS = 10,     REFV9 = 10
16 : AW_9VOLTS =  16,      BW_9VOLTS = 16,       AVS9VOLTS = 16,       REFV9 = 16
32 : AW_9VOLTS =  32,      BW_9VOLTS = 32,       AVS9VOLTS = 32,       REFV9 = 32
64 : AW_9VOLTS =  64,      BW_9VOLTS = 64,       AVS9VOLTS = 64,       REFV9 = 64
100 : AW_9VOLTS = 100,     BW_9VOLTS = 100,     AVS9VOLTS = 100,     REFV9 = 100
128 : AW_9VOLTS =  128,      BW_9VOLTS = 128,       AVS9VOLTS = 128,       REFV9 = 128
256 : AW_9VOLTS =  256,      BW_9VOLTS = 256,       AVS9VOLTS = 256,       REFV9 = 256
512 : AW_9VOLTS =  512,      BW_9VOLTS = 512,       AVS9VOLTS = 512,       REFV9 = 512
655.35 : AW_9VOLTS =  655.35, BW_9VOLTS = 655.35,  AVS9VOLTS = 655.35,  REFV9 = 655.35
1000 : AW_9VOLTS = 1000,     BW_9VOLTS = 1000,     AVS9VOLTS = 1000,     REFV9 = 1000
1024 : AW_9VOLTS =  1024,    BW_9VOLTS = 1024,     AVS9VOLTS = 1024,     REFV9 = 1024
10000 : AW_9VOLTS = 10000,     BW_9VOLTS = 10000,     AVS9VOLTS = 10000,     REFV9 = 10000
32768 : AW_9VOLTS =  32768,  BW_9VOLTS = 32768,   AVS9VOLTS = 32768,   REFV9 = 32768
65535 : AW_9VOLTS =  65535,  BW_9VOLTS = 65535,   AVS9VOLTS = 65535,   REFV9 = 65535

*MAPPINGS,14,STEP10
10 : AW_10VOLTS = 10,     BW_10VOLTS = 10,     AVS10VOLTS = 10,     REFV10 = 10
16 : AW_10VOLTS =  16,      BW_10VOLTS = 16,       AVS10VOLTS = 16,       REFV10 = 16
32 : AW_10VOLTS =  32,      BW_10VOLTS = 32,       AVS10VOLTS = 32,       REFV10 = 32
64 : AW_10VOLTS =  64,      BW_10VOLTS = 64,       AVS10VOLTS = 64,       REFV10 = 64
100 : AW_10VOLTS = 100,     BW_10VOLTS = 100,     AVS10VOLTS = 100,     REFV10 = 100
128 : AW_10VOLTS =  128,      BW_10VOLTS = 128,       AVS10VOLTS = 128,       REFV10 = 128
256 : AW_10VOLTS =  256,      BW_10VOLTS = 256,       AVS10VOLTS = 256,       REFV10 = 256
512 : AW_10VOLTS =  512,      BW_10VOLTS = 512,       AVS10VOLTS = 512,       REFV10 = 512
655.35 : AW_10VOLTS =  655.35, BW_10VOLTS = 655.35,  AVS10VOLTS = 655.35,  REFV10 = 655.35
1000 : AW_10VOLTS = 1000,     BW_10VOLTS = 1000,     AVS10VOLTS = 1000,     REFV10 = 1000
1024 : AW_10VOLTS =  1024,    BW_10VOLTS = 1024,     AVS10VOLTS = 1024,     REFV10 = 1024
10000 : AW_10VOLTS = 10000,     BW_10VOLTS = 10000,     AVS10VOLTS = 10000,     REFV10 = 10000
32768 : AW_10VOLTS =  32768,  BW_10VOLTS = 32768,   AVS10VOLTS = 32768,   REFV10 = 32768
65535 : AW_10VOLTS =  65535,  BW_10VOLTS = 65535,   AVS10VOLTS = 65535,   REFV10 = 65535

*MAPPINGS,14,STEP11
10 : AW_11VOLTS = 10,     BW_11VOLTS = 10,     AVS11VOLTS = 10,     REFV11 = 10
16 : AW_11VOLTS =  16,      BW_11VOLTS = 16,       AVS11VOLTS = 16,       REFV11 = 16
32 : AW_11VOLTS =  32,      BW_11VOLTS = 32,       AVS11VOLTS = 32,       REFV11 = 32
64 : AW_11VOLTS =  64,      BW_11VOLTS = 64,       AVS11VOLTS = 64,       REFV11 = 64
100 : AW_11VOLTS = 100,     BW_11VOLTS = 100,     AVS11VOLTS = 100,     REFV11 = 100
128 : AW_11VOLTS =  128,      BW_11VOLTS = 128,       AVS11VOLTS = 128,       REFV11 = 128
256 : AW_11VOLTS =  256,      BW_11VOLTS = 256,       AVS11VOLTS = 256,       REFV11 = 256
512 : AW_11VOLTS =  512,      BW_11VOLTS = 512,       AVS11VOLTS = 512,       REFV11 = 512
655.35 : AW_11VOLTS =  655.35, BW_11VOLTS = 655.35,  AVS11VOLTS = 655.35,  REFV11 = 655.35
1000 : AW_11VOLTS = 1000,     BW_11VOLTS = 1000,     AVS11VOLTS = 1000,     REFV11 = 1000
1024 : AW_11VOLTS =  1024,    BW_11VOLTS = 1024,     AVS11VOLTS = 1024,     REFV11 = 1024
10000 : AW_11VOLTS = 10000,     BW_11VOLTS = 10000,     AVS11VOLTS = 10000,     REFV11 = 10000
32768 : AW_11VOLTS =  32768,  BW_11VOLTS = 32768,   AVS11VOLTS = 32768,   REFV11 = 32768
65535 : AW_11VOLTS =  65535,  BW_11VOLTS = 65535,   AVS11VOLTS = 65535,   REFV11 = 65535

*MAPPINGS,14,STEP12
10 : AW_12VOLTS = 10,     BW_12VOLTS = 10,     AVS12VOLTS = 10,     REFV12 = 10
16 : AW_12VOLTS =  16,      BW_12VOLTS = 16,       AVS12VOLTS = 16,       REFV12 = 16
32 : AW_12VOLTS =  32,      BW_12VOLTS = 32,       AVS12VOLTS = 32,       REFV12 = 32
64 : AW_12VOLTS =  64,      BW_12VOLTS = 64,       AVS12VOLTS = 64,       REFV12 = 64
100 : AW_12VOLTS = 100,     BW_12VOLTS = 100,     AVS12VOLTS = 100,     REFV12 = 100
128 : AW_12VOLTS =  128,      BW_12VOLTS = 128,       AVS12VOLTS = 128,       REFV12 = 128
256 : AW_12VOLTS =  256,      BW_12VOLTS = 256,       AVS12VOLTS = 256,       REFV12 = 256
512 : AW_12VOLTS =  512,      BW_12VOLTS = 512,       AVS12VOLTS = 512,       REFV12 = 512
655.35 : AW_12VOLTS =  655.35, BW_12VOLTS = 655.35,  AVS12VOLTS = 655.35,  REFV12 = 655.35
1000 : AW_12VOLTS = 1000,     BW_12VOLTS = 1000,     AVS12VOLTS = 1000,     REFV12 = 1000
1024 : AW_12VOLTS =  1024,    BW_12VOLTS = 1024,     AVS12VOLTS = 1024,     REFV12 = 1024
10000 : AW_12VOLTS = 10000,     BW_12VOLTS = 10000,     AVS12VOLTS = 10000,     REFV12 = 10000
32768 : AW_12VOLTS =  32768,  BW_12VOLTS = 32768,   AVS12VOLTS = 32768,   REFV12 = 32768
65535 : AW_12VOLTS =  65535,  BW_12VOLTS = 65535,   AVS12VOLTS = 65535,   REFV12 = 65535

*MAPPINGS,14,STEP13
10 : AW_13VOLTS = 10,     BW_13VOLTS = 10,     AVS13VOLTS = 10,     REFV13 = 10
16 : AW_13VOLTS =  16,      BW_13VOLTS = 16,       AVS13VOLTS = 16,       REFV13 = 16
32 : AW_13VOLTS =  32,      BW_13VOLTS = 32,       AVS13VOLTS = 32,       REFV13 = 32
64 : AW_13VOLTS =  64,      BW_13VOLTS = 64,       AVS13VOLTS = 64,       REFV13 = 64
100 : AW_13VOLTS = 100,     BW_13VOLTS = 100,     AVS13VOLTS = 100,     REFV13 = 100
128 : AW_13VOLTS =  128,      BW_13VOLTS = 128,       AVS13VOLTS = 128,       REFV13 = 128
256 : AW_13VOLTS =  256,      BW_13VOLTS = 256,       AVS13VOLTS = 256,       REFV13 = 256
512 : AW_13VOLTS =  512,      BW_13VOLTS = 512,       AVS13VOLTS = 512,       REFV13 = 512
655.35 : AW_13VOLTS =  655.35, BW_13VOLTS = 655.35,  AVS13VOLTS = 655.35,  REFV13 = 655.35
1000 : AW_13VOLTS = 1000,     BW_13VOLTS = 1000,     AVS13VOLTS = 1000,     REFV13 = 1000
1024 : AW_13VOLTS =  1024,    BW_13VOLTS = 1024,     AVS13VOLTS = 1024,     REFV13 = 1024
10000 : AW_13VOLTS = 10000,     BW_13VOLTS = 10000,     AVS13VOLTS = 10000,     REFV13 = 10000
32768 : AW_13VOLTS =  32768,  BW_13VOLTS = 32768,   AVS13VOLTS = 32768,   REFV13 = 32768
65535 : AW_13VOLTS =  65535,  BW_13VOLTS = 65535,   AVS13VOLTS = 65535,   REFV13 = 65535

*MAPPINGS,14,STEP14
10 : AW_14VOLTS = 10,     BW_14VOLTS = 10,     AVS14VOLTS = 10,     REFV14 = 10
16 : AW_14VOLTS =  16,      BW_14VOLTS = 16,       AVS14VOLTS = 16,       REFV14 = 16
32 : AW_14VOLTS =  32,      BW_14VOLTS = 32,       AVS14VOLTS = 32,       REFV14 = 32
64 : AW_14VOLTS =  64,      BW_14VOLTS = 64,       AVS14VOLTS = 64,       REFV14 = 64
100 : AW_14VOLTS = 100,     BW_14VOLTS = 100,     AVS14VOLTS = 100,     REFV14 = 100
128 : AW_14VOLTS =  128,      BW_14VOLTS = 128,       AVS14VOLTS = 128,       REFV14 = 128
256 : AW_14VOLTS =  256,      BW_14VOLTS = 256,       AVS14VOLTS = 256,       REFV14 = 256
512 : AW_14VOLTS =  512,      BW_14VOLTS = 512,       AVS14VOLTS = 512,       REFV14 = 512
655.35 : AW_14VOLTS =  655.35, BW_14VOLTS = 655.35,  AVS14VOLTS = 655.35,  REFV14 = 655.35
1000 : AW_14VOLTS = 1000,     BW_14VOLTS = 1000,     AVS14VOLTS = 1000,     REFV14 = 1000
1024 : AW_14VOLTS =  1024,    BW_14VOLTS = 1024,     AVS14VOLTS = 1024,     REFV14 = 1024
10000 : AW_14VOLTS = 10000,     BW_14VOLTS = 10000,     AVS14VOLTS = 10000,     REFV14 = 10000
32768 : AW_14VOLTS =  32768,  BW_14VOLTS = 32768,   AVS14VOLTS = 32768,   REFV14 = 32768
65535 : AW_14VOLTS =  65535,  BW_14VOLTS = 65535,   AVS14VOLTS = 65535,   REFV14 = 65535

*MAPPINGS,14,STEP15
10 : AW_15VOLTS = 10,     BW_15VOLTS = 10,     AVS15VOLTS = 10,     REFV15 = 10
16 : AW_15VOLTS =  16,      BW_15VOLTS = 16,       AVS15VOLTS = 16,       REFV15 = 16
32 : AW_15VOLTS =  32,      BW_15VOLTS = 32,       AVS15VOLTS = 32,       REFV15 = 32
64 : AW_15VOLTS =  64,      BW_15VOLTS = 64,       AVS15VOLTS = 64,       REFV15 = 64
100 : AW_15VOLTS = 100,     BW_15VOLTS = 100,     AVS15VOLTS = 100,     REFV15 = 100
128 : AW_15VOLTS =  128,      BW_15VOLTS = 128,       AVS15VOLTS = 128,       REFV15 = 128
256 : AW_15VOLTS =  256,      BW_15VOLTS = 256,       AVS15VOLTS = 256,       REFV15 = 256
512 : AW_15VOLTS =  512,      BW_15VOLTS = 512,       AVS15VOLTS = 512,       REFV15 = 512
655.35 : AW_15VOLTS =  655.35, BW_15VOLTS = 655.35,  AVS15VOLTS = 655.35,  REFV15 = 655.35
1000 : AW_15VOLTS = 1000,     BW_15VOLTS = 1000,     AVS15VOLTS = 1000,     REFV15 = 1000
1024 : AW_15VOLTS =  1024,    BW_15VOLTS = 1024,     AVS15VOLTS = 1024,     REFV15 = 1024
10000 : AW_15VOLTS = 10000,     BW_15VOLTS = 10000,     AVS15VOLTS = 10000,     REFV15 = 10000
32768 : AW_15VOLTS =  32768,  BW_15VOLTS = 32768,   AVS15VOLTS = 32768,   REFV15 = 32768
65535 : AW_15VOLTS =  65535,  BW_15VOLTS = 65535,   AVS15VOLTS = 65535,   REFV15 = 65535

*MAPPINGS,14,STEP16
10 : AW_16VOLTS = 10,     BW_16VOLTS = 10,     AVS16VOLTS = 10,     REFV16 = 10
16 : AW_16VOLTS =  16,      BW_16VOLTS = 16,       AVS16VOLTS = 16,       REFV16 = 16
32 : AW_16VOLTS =  32,      BW_16VOLTS = 32,       AVS16VOLTS = 32,       REFV16 = 32
64 : AW_16VOLTS =  64,      BW_16VOLTS = 64,       AVS16VOLTS = 64,       REFV16 = 64
100 : AW_16VOLTS = 100,     BW_16VOLTS = 100,     AVS16VOLTS = 100,     REFV16 = 100
128 : AW_16VOLTS =  128,      BW_16VOLTS = 128,       AVS16VOLTS = 128,       REFV16 = 128
256 : AW_16VOLTS =  256,      BW_16VOLTS = 256,       AVS16VOLTS = 256,       REFV16 = 256
512 : AW_16VOLTS =  512,      BW_16VOLTS = 512,       AVS16VOLTS = 512,       REFV16 = 512
655.35 : AW_16VOLTS =  655.35, BW_16VOLTS = 655.35,  AVS16VOLTS = 655.35,  REFV16 = 655.35
1000 : AW_16VOLTS = 1000,     BW_16VOLTS = 1000,     AVS16VOLTS = 1000,     REFV16 = 1000
1024 : AW_16VOLTS =  1024,    BW_16VOLTS = 1024,     AVS16VOLTS = 1024,     REFV16 = 1024
10000 : AW_16VOLTS = 10000,     BW_16VOLTS = 10000,     AVS16VOLTS = 10000,     REFV16 = 10000
32768 : AW_16VOLTS =  32768,  BW_16VOLTS = 32768,   AVS16VOLTS = 32768,   REFV16 = 32768
65535 : AW_16VOLTS =  65535,  BW_16VOLTS = 65535,   AVS16VOLTS = 65535,   REFV16 = 65535

*MODELDEFS,0    

*PARTLIST,194  
DBNK1_SW1,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW2,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW3,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW4,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW5,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW6,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW7,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW8,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW9,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW10,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW11,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW12,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW13,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW14,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW15,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW16,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
VBNK1_V1,VSOURCE,<REFV1>,PRIMITIVE=ANALOG
VBNK1_V2,VSOURCE,<REFV2>,PRIMITIVE=ANALOG
VBNK1_V3,VSOURCE,<REFV3>,PRIMITIVE=ANALOG
VBNK1_V4,VSOURCE,<REFV4>,PRIMITIVE=ANALOG
VBNK2_V1,VSOURCE,<REFV5>,PRIMITIVE=ANALOG
VBNK2_V2,VSOURCE,<REFV6>,PRIMITIVE=ANALOG
VBNK2_V3,VSOURCE,<REFV7>,PRIMITIVE=ANALOG
VBNK2_V4,VSOURCE,<REFV8>,PRIMITIVE=ANALOG
VBNK3_V1,VSOURCE,<REFV9>,PRIMITIVE=ANALOG
VBNK3_V2,VSOURCE,<REFV10>,PRIMITIVE=ANALOG
VBNK3_V3,VSOURCE,<REFV11>,PRIMITIVE=ANALOG
VBNK3_V4,VSOURCE,<REFV12>,PRIMITIVE=ANALOG
VBNK4_V1,VSOURCE,<REFV13>,PRIMITIVE=ANALOG
VBNK4_V2,VSOURCE,<REFV14>,PRIMITIVE=ANALOG
VBNK4_V3,VSOURCE,<REFV15>,PRIMITIVE=ANALOG
VBNK4_V4,VSOURCE,<REFV16>,PRIMITIVE=ANALOG
VCP1_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP1_AVS2,AVS,"<AVS1VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP1_C1,CAPACITOR,<GCPP1>,PRIMITIVE=ANALOGUE
VCP1_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP1_R2,RESISTOR,<GR1>,PRIMITIVE=ANALOGUE
VCP1_R3,RESISTOR,<GR1>,PRIMITIVE=ANALOGUE
VCP1_R4,RESISTOR,<GR1>,PRIMITIVE=ANALOGUE
VCP1_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL1>,RON=1p,VOFF=0,VON=<BW_1VOLTS>
VCP1_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL1>,RON=1p,VOFF=0,VON=<AW_1VOLTS>
VCP10_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP10_AVS2,AVS,"<AVS10VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP10_C1,CAPACITOR,<GCPP10>,PRIMITIVE=ANALOGUE
VCP10_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP10_R2,RESISTOR,<GR10>,PRIMITIVE=ANALOGUE
VCP10_R3,RESISTOR,<GR10>,PRIMITIVE=ANALOGUE
VCP10_R4,RESISTOR,<GR10>,PRIMITIVE=ANALOGUE
VCP10_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL10>,RON=1p,VOFF=0,VON=<BW_10VOLTS>
VCP10_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL10>,RON=1p,VOFF=0,VON=<AW_10VOLTS>
VCP11_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP11_AVS2,AVS,"<AVS11VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP11_C1,CAPACITOR,<GCPP11>,PRIMITIVE=ANALOGUE
VCP11_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP11_R2,RESISTOR,<GR11>,PRIMITIVE=ANALOGUE
VCP11_R3,RESISTOR,<GR11>,PRIMITIVE=ANALOGUE
VCP11_R4,RESISTOR,<GR11>,PRIMITIVE=ANALOGUE
VCP11_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL11>,RON=1p,VOFF=0,VON=<BW_11VOLTS>
VCP11_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL11>,RON=1p,VOFF=0,VON=<AW_11VOLTS>
VCP12_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP12_AVS2,AVS,"<AVS12VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP12_C1,CAPACITOR,<GCPP12>,PRIMITIVE=ANALOGUE
VCP12_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP12_R2,RESISTOR,<GR12>,PRIMITIVE=ANALOGUE
VCP12_R3,RESISTOR,<GR12>,PRIMITIVE=ANALOGUE
VCP12_R4,RESISTOR,<GR12>,PRIMITIVE=ANALOGUE
VCP12_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL12>,RON=1p,VOFF=0,VON=<BW_12VOLTS>
VCP12_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL12>,RON=1p,VOFF=0,VON=<AW_12VOLTS>
VCP13_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP13_AVS2,AVS,"<AVS13VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP13_C1,CAPACITOR,<GCPP13>,PRIMITIVE=ANALOGUE
VCP13_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP13_R2,RESISTOR,<GR13>,PRIMITIVE=ANALOGUE
VCP13_R3,RESISTOR,<GR13>,PRIMITIVE=ANALOGUE
VCP13_R4,RESISTOR,<GR13>,PRIMITIVE=ANALOGUE
VCP13_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL13>,RON=1p,VOFF=0,VON=<BW_13VOLTS>
VCP13_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL13>,RON=1p,VOFF=0,VON=<AW_13VOLTS>
VCP14_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP14_AVS2,AVS,"<AVS14VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP14_C1,CAPACITOR,<GCPP14>,PRIMITIVE=ANALOGUE
VCP14_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP14_R2,RESISTOR,<GR14>,PRIMITIVE=ANALOGUE
VCP14_R3,RESISTOR,<GR14>,PRIMITIVE=ANALOGUE
VCP14_R4,RESISTOR,<GR14>,PRIMITIVE=ANALOGUE
VCP14_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL14>,RON=1p,VOFF=0,VON=<BW_14VOLTS>
VCP14_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL14>,RON=1p,VOFF=0,VON=<AW_14VOLTS>
VCP15_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP15_AVS2,AVS,"<AVS15VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP15_C1,CAPACITOR,<GCPP15>,PRIMITIVE=ANALOGUE
VCP15_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP15_R2,RESISTOR,<GR15>,PRIMITIVE=ANALOGUE
VCP15_R3,RESISTOR,<GR15>,PRIMITIVE=ANALOGUE
VCP15_R4,RESISTOR,<GR15>,PRIMITIVE=ANALOGUE
VCP15_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL15>,RON=1p,VOFF=0,VON=<BW_15VOLTS>
VCP15_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL15>,RON=1p,VOFF=0,VON=<AW_15VOLTS>
VCP16_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP16_AVS2,AVS,"<AVS16VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP16_C1,CAPACITOR,<GCPP16>,PRIMITIVE=ANALOGUE
VCP16_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP16_R2,RESISTOR,<GR16>,PRIMITIVE=ANALOGUE
VCP16_R3,RESISTOR,<GR16>,PRIMITIVE=ANALOGUE
VCP16_R4,RESISTOR,<GR16>,PRIMITIVE=ANALOGUE
VCP16_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL16>,RON=1p,VOFF=0,VON=<BW_16VOLTS>
VCP16_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL16>,RON=1p,VOFF=0,VON=<AW_16VOLTS>
VCP2_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP2_AVS2,AVS,"<AVS2VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP2_C1,CAPACITOR,<GCPP2>,PRIMITIVE=ANALOGUE
VCP2_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP2_R2,RESISTOR,<GR2>,PRIMITIVE=ANALOGUE
VCP2_R3,RESISTOR,<GR2>,PRIMITIVE=ANALOGUE
VCP2_R4,RESISTOR,<GR2>,PRIMITIVE=ANALOGUE
VCP2_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL2>,RON=1p,VOFF=0,VON=<BW_2VOLTS>
VCP2_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL2>,RON=1p,VOFF=0,VON=<AW_2VOLTS>
VCP3_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP3_AVS2,AVS,"<AVS3VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP3_C1,CAPACITOR,<GCPP3>,PRIMITIVE=ANALOGUE
VCP3_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP3_R2,RESISTOR,<GR3>,PRIMITIVE=ANALOGUE
VCP3_R3,RESISTOR,<GR3>,PRIMITIVE=ANALOGUE
VCP3_R4,RESISTOR,<GR3>,PRIMITIVE=ANALOGUE
VCP3_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL3>,RON=1p,VOFF=0,VON=<BW_3VOLTS>
VCP3_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL3>,RON=1p,VOFF=0,VON=<AW_3VOLTS>
VCP4_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP4_AVS2,AVS,"<AVS4VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP4_C1,CAPACITOR,<GCPP4>,PRIMITIVE=ANALOGUE
VCP4_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP4_R2,RESISTOR,<GR4>,PRIMITIVE=ANALOGUE
VCP4_R3,RESISTOR,<GR4>,PRIMITIVE=ANALOGUE
VCP4_R4,RESISTOR,<GR4>,PRIMITIVE=ANALOGUE
VCP4_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL4>,RON=1p,VOFF=0,VON=<BW_4VOLTS>
VCP4_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL4>,RON=1p,VOFF=0,VON=<AW_4VOLTS>
VCP5_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP5_AVS2,AVS,"<AVS5VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP5_C1,CAPACITOR,<GCPP5>,PRIMITIVE=ANALOGUE
VCP5_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP5_R2,RESISTOR,<GR5>,PRIMITIVE=ANALOGUE
VCP5_R3,RESISTOR,<GR5>,PRIMITIVE=ANALOGUE
VCP5_R4,RESISTOR,<GR5>,PRIMITIVE=ANALOGUE
VCP5_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL5>,RON=1p,VOFF=0,VON=<BW_5VOLTS>
VCP5_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL5>,RON=1p,VOFF=0,VON=<AW_5VOLTS>
VCP6_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP6_AVS2,AVS,"<AVS6VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP6_C1,CAPACITOR,<GCPP6>,PRIMITIVE=ANALOGUE
VCP6_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP6_R2,RESISTOR,<GR6>,PRIMITIVE=ANALOGUE
VCP6_R3,RESISTOR,<GR6>,PRIMITIVE=ANALOGUE
VCP6_R4,RESISTOR,<GR6>,PRIMITIVE=ANALOGUE
VCP6_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL6>,RON=1p,VOFF=0,VON=<BW_6VOLTS>
VCP6_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL6>,RON=1p,VOFF=0,VON=<AW_6VOLTS>
VCP7_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP7_AVS2,AVS,"<AVS7VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP7_C1,CAPACITOR,<GCPP7>,PRIMITIVE=ANALOGUE
VCP7_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP7_R2,RESISTOR,<GR7>,PRIMITIVE=ANALOGUE
VCP7_R3,RESISTOR,<GR7>,PRIMITIVE=ANALOGUE
VCP7_R4,RESISTOR,<GR7>,PRIMITIVE=ANALOGUE
VCP7_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL7>,RON=1p,VOFF=0,VON=<BW_7VOLTS>
VCP7_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL7>,RON=1p,VOFF=0,VON=<AW_7VOLTS>
VCP8_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP8_AVS2,AVS,"<AVS8VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP8_C1,CAPACITOR,<GCPP8>,PRIMITIVE=ANALOGUE
VCP8_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP8_R2,RESISTOR,<GR8>,PRIMITIVE=ANALOGUE
VCP8_R3,RESISTOR,<GR8>,PRIMITIVE=ANALOGUE
VCP8_R4,RESISTOR,<GR8>,PRIMITIVE=ANALOGUE
VCP8_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL8>,RON=1p,VOFF=0,VON=<BW_8VOLTS>
VCP8_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL8>,RON=1p,VOFF=0,VON=<AW_8VOLTS>
VCP9_AVS1,AVS,"1.0*V(A,B)",PRIMITIVE=ANALOGUE
VCP9_AVS2,AVS,"<AVS9VOLTS>-V(A,B)",PRIMITIVE=ANALOGUE
VCP9_C1,CAPACITOR,<GCPP9>,PRIMITIVE=ANALOGUE
VCP9_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP9_R2,RESISTOR,<GR9>,PRIMITIVE=ANALOGUE
VCP9_R3,RESISTOR,<GR9>,PRIMITIVE=ANALOGUE
VCP9_R4,RESISTOR,<GR9>,PRIMITIVE=ANALOGUE
VCP9_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL9>,RON=1p,VOFF=0,VON=<BW_9VOLTS>
VCP9_S2,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=<POTVAL9>,RON=1p,VOFF=0,VON=<AW_9VOLTS>
CLOCK#0020,DIGITAL!,,CLOCK=<APUDFREQ>,INIT=0,PRIMITIVE=DIGITAL
COMVDDINTRN#001F,COMVDD,,BTE=<BTE>,BTSWITCH=<BTSWITCH>,BUTTONS=<BUTTONS>,CRM=<CRM>,DEC=<DEC>,DECADE=<DECADE>,DM=<DM>,DS=<DS>,ENSAVED=<ENSAVED>,HIDEOA=<HIDEOA>,INITBTNS=<INITBTNS>,INITSW=<INITSW>,MODDLL=COMVDD,PRERETRY=<PRERETRY>,PRIMITIVE=DIGITAL,PSDELAY=<PSDELAY>,ptCONV=<ptCONV>,PTM=<PTM>,PUVIEW=<PUVIEW>,SDSSW=<SDSSW>,SHMEM=<SHMEM>,SIMRETRY=<SIMRETRY>,SLIDERS=<SLIDERS>,SPRINGEN=<SPRINGEN>,SSDELAY=<SSDELAY>,SSPU=<SSPU>,STSWITCH=<STSWITCH>,SWITCHES=<SWITCHES>,tsbCONV=<tsbCONV>,VD_BAUDRATE=<VD_BAUDRATE>,VD_DATABITS=<VD_DATABITS>,VD_PARITY=<VD_PARITY>,VD_PORT=<VD_PORT>,VD_STOPBITS=<VD_STOPBITS>,VDD=<VDD>,XPOTS=<XPOTS>
R1,RES,<GR1>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R2,RES,<GR2>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R3,RES,<GR3>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R4,RES,<GR4>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R5,RES,<GR9>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R6,RES,<GR10>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R7,RES,<GR11>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R8,RES,<GR12>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R9,RES,<GR13>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R10,RES,<GR14>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R11,RES,<GR15>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R12,RES,<GR16>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R13,RES,<GR8>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R14,RES,<GR7>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R15,RES,<GR6>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R16,RES,<GR6>,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR

*NETLIST,175  
#00000,2
COMVDDINTRN#001F,PS,PUDCLK
CLOCK#0020,OP,*

#00001,1
COMVDDINTRN#001F,OP,HOLDV

#00002,2
VCP1_S1,PS,P
VCP1_AVS1,PS,+

#00003,2
VCP1_S2,PS,P
VCP1_AVS2,PS,+

#00004,2
VCP2_S1,PS,P
VCP2_AVS1,PS,+

#00005,2
VCP2_S2,PS,P
VCP2_AVS2,PS,+

#00006,2
VCP3_S1,PS,P
VCP3_AVS1,PS,+

#00007,2
VCP3_S2,PS,P
VCP3_AVS2,PS,+

#00008,2
VCP4_S1,PS,P
VCP4_AVS1,PS,+

#00009,2
VCP4_S2,PS,P
VCP4_AVS2,PS,+

#00010,2
VCP5_S1,PS,P
VCP5_AVS1,PS,+

#00011,2
VCP5_S2,PS,P
VCP5_AVS2,PS,+

#00012,2
VCP6_S1,PS,P
VCP6_AVS1,PS,+

#00013,2
VCP6_S2,PS,P
VCP6_AVS2,PS,+

#00014,2
VCP7_S1,PS,P
VCP7_AVS1,PS,+

#00015,2
VCP7_S2,PS,P
VCP7_AVS2,PS,+

#00016,2
VCP8_S1,PS,P
VCP8_AVS1,PS,+

#00017,2
VCP8_S2,PS,P
VCP8_AVS2,PS,+

#00018,2
VCP9_S1,PS,P
VCP9_AVS1,PS,+

#00019,2
VCP9_S2,PS,P
VCP9_AVS2,PS,+

#00020,2
VCP10_S1,PS,P
VCP10_AVS1,PS,+

#00021,2
VCP10_S2,PS,P
VCP10_AVS2,PS,+

#00022,2
VCP11_S1,PS,P
VCP11_AVS1,PS,+

#00023,2
VCP11_S2,PS,P
VCP11_AVS2,PS,+

#00024,2
VCP12_S1,PS,P
VCP12_AVS1,PS,+

#00025,2
VCP12_S2,PS,P
VCP12_AVS2,PS,+

#00026,2
VCP13_S1,PS,P
VCP13_AVS1,PS,+

#00027,2
VCP13_S2,PS,P
VCP13_AVS2,PS,+

#00028,2
VCP14_S1,PS,P
VCP14_AVS1,PS,+

#00029,2
VCP14_S2,PS,P
VCP14_AVS2,PS,+

#00030,2
VCP15_S1,PS,P
VCP15_AVS1,PS,+

#00031,2
VCP15_S2,PS,P
VCP15_AVS2,PS,+

#00032,2
VCP16_S1,PS,P
VCP16_AVS1,PS,+

#00033,2
VCP16_S2,PS,P
VCP16_AVS2,PS,+

BTND_COM,2
BTND_COM,IT
COMVDDINTRN#001F,PS,BTN_COM

RESET,2
RESET,IT
COMVDDINTRN#001F,PS,RESET

SWD_COM,2
SWD_COM,IT
COMVDDINTRN#001F,PS,SW_COM

SAVE,2
SAVE,IT
COMVDDINTRN#001F,PS,SAVE

BTN_COM1,3
BTN_COM1,GT
DBNK1_SW1,IO,A
DBNK1_SW2,IO,A

B1TN1,2
B1TN1,GT
DBNK1_SW1,IO,B

BTND1,3
BTND1,OT
DBNK1_SW1,IP,EN
COMVDDINTRN#001F,IO,BTN1

B1TN2,2
B1TN2,GT
DBNK1_SW2,IO,B

BTND2,3
BTND2,OT
DBNK1_SW2,IP,EN
COMVDDINTRN#001F,IO,BTN2

BTN_COM2,3
BTN_COM2,GT
DBNK1_SW3,IO,A
DBNK1_SW4,IO,A

B2TN3,2
B2TN3,GT
DBNK1_SW3,IO,B

BTND3,3
BTND3,OT
DBNK1_SW3,IP,EN
COMVDDINTRN#001F,IO,BTN3

B2TN4,2
B2TN4,GT
DBNK1_SW4,IO,B

BTND4,3
BTND4,OT
DBNK1_SW4,IP,EN
COMVDDINTRN#001F,IO,BTN4

BTN_COM3,3
BTN_COM3,GT
DBNK1_SW5,IO,A
DBNK1_SW6,IO,A

B3TN5,2
B3TN5,GT
DBNK1_SW5,IO,B

BTND5,3
BTND5,OT
DBNK1_SW5,IP,EN
COMVDDINTRN#001F,IO,BTN5

B3TN6,2
B3TN6,GT
DBNK1_SW6,IO,B

BTND6,3
BTND6,OT
DBNK1_SW6,IP,EN
COMVDDINTRN#001F,IO,BTN6

BTN_COM4,3
BTN_COM4,GT
DBNK1_SW7,IO,A
DBNK1_SW8,IO,A

B4TN7,2
B4TN7,GT
DBNK1_SW7,IO,B

BTND7,3
BTND7,OT
DBNK1_SW7,IP,EN
COMVDDINTRN#001F,IO,BTN7

B4TN8,2
B4TN8,GT
DBNK1_SW8,IO,B

BTND8,3
BTND8,OT
DBNK1_SW8,IP,EN
COMVDDINTRN#001F,IO,BTN8

SW_COM1,3
SW_COM1,GT
DBNK1_SW9,IO,A
DBNK1_SW10,IO,A

S1W1,2
S1W1,GT
DBNK1_SW9,IO,B

SWD1,3
SWD1,OT
DBNK1_SW9,IP,EN
COMVDDINTRN#001F,IO,SW1

S1W2,2
S1W2,GT
DBNK1_SW10,IO,B

SWD2,3
SWD2,OT
DBNK1_SW10,IP,EN
COMVDDINTRN#001F,IO,SW2

SW_COM2,3
SW_COM2,GT
DBNK1_SW11,IO,A
DBNK1_SW12,IO,A

S2W3,2
S2W3,GT
DBNK1_SW11,IO,B

SWD3,3
SWD3,OT
DBNK1_SW11,IP,EN
COMVDDINTRN#001F,IO,SW3

S2W4,2
S2W4,GT
DBNK1_SW12,IO,B

SWD4,3
SWD4,OT
DBNK1_SW12,IP,EN
COMVDDINTRN#001F,IO,SW4

SW_COM3,3
SW_COM3,GT
DBNK1_SW13,IO,A
DBNK1_SW14,IO,A

S3W5,2
S3W5,GT
DBNK1_SW13,IO,B

SWD5,3
SWD5,OT
DBNK1_SW13,IP,EN
COMVDDINTRN#001F,IO,SW5

S3W6,2
S3W6,GT
DBNK1_SW14,IO,B

SWD6,3
SWD6,OT
DBNK1_SW14,IP,EN
COMVDDINTRN#001F,IO,SW6

SW_COM4,3
SW_COM4,GT
DBNK1_SW15,IO,A
DBNK1_SW16,IO,A

S4W7,2
S4W7,GT
DBNK1_SW15,IO,B

SWD7,3
SWD7,OT
DBNK1_SW15,IP,EN
COMVDDINTRN#001F,IO,SW7

S4W8,2
S4W8,GT
DBNK1_SW16,IO,B

SWD8,3
SWD8,OT
DBNK1_SW16,IP,EN
COMVDDINTRN#001F,IO,SW8

#00034,2
VBNK1_V1,PS,+
COMVDDINTRN#001F,PS,POT1R

#00035,2
VBNK1_V2,PS,+
COMVDDINTRN#001F,PS,POT2R

#00036,2
VBNK1_V3,PS,+
COMVDDINTRN#001F,PS,POT3R

#00037,2
VBNK1_V4,PS,+
COMVDDINTRN#001F,PS,POT4R

#00038,2
VBNK2_V1,PS,+
COMVDDINTRN#001F,PS,POT5R

#00039,2
VBNK2_V2,PS,+
COMVDDINTRN#001F,PS,POT6R

#00040,2
VBNK2_V3,PS,+
COMVDDINTRN#001F,PS,POT7R

#00041,2
VBNK2_V4,PS,+
COMVDDINTRN#001F,PS,POT8R

#00042,2
VBNK3_V1,PS,+
COMVDDINTRN#001F,PS,POT9R

#00043,2
VBNK3_V2,PS,+
COMVDDINTRN#001F,PS,POT10R

#00044,2
VBNK3_V3,PS,+
COMVDDINTRN#001F,PS,POT11R

#00045,2
VBNK3_V4,PS,+
COMVDDINTRN#001F,PS,POT12R

#00046,2
VBNK4_V1,PS,+
COMVDDINTRN#001F,PS,POT13R

#00047,2
VBNK4_V2,PS,+
COMVDDINTRN#001F,PS,POT14R

#00048,2
VBNK4_V3,PS,+
COMVDDINTRN#001F,PS,POT15R

#00049,2
VBNK4_V4,PS,+
COMVDDINTRN#001F,PS,POT16R

POT1_B,3
POT1_B,GT
VCP1_S1,PS,+
VCP1_R4,PS,2

POT1_C,4
POT1_C,GT
VCP1_S1,PS,-
VCP1_S2,PS,-
VCP1_R3,PS,2

POT1_A,3
POT1_A,GT
VCP1_S2,PS,+
VCP1_R2,PS,2

#00050,4
VCP1_AVS1,PS,A
VCP1_AVS2,PS,A
VCP1_R1,PS,2
COMVDDINTRN#001F,PS,POT1V

AGND1,6
AGND1,GT
VCP1_R2,PS,1
VCP1_R3,PS,1
VCP1_R4,PS,1
VCP1_C1,PS,1
R1,PS,2

POT2_B,3
POT2_B,GT
VCP2_S1,PS,+
VCP2_R4,PS,2

POT2_C,4
POT2_C,GT
VCP2_S1,PS,-
VCP2_S2,PS,-
VCP2_R3,PS,2

POT2_A,3
POT2_A,GT
VCP2_S2,PS,+
VCP2_R2,PS,2

#00051,4
VCP2_AVS1,PS,A
VCP2_AVS2,PS,A
VCP2_R1,PS,2
COMVDDINTRN#001F,PS,POT2V

AGND2,6
AGND2,GT
VCP2_R2,PS,1
VCP2_R3,PS,1
VCP2_R4,PS,1
VCP2_C1,PS,1
R2,PS,2

POT3_B,3
POT3_B,GT
VCP3_S1,PS,+
VCP3_R4,PS,2

POT3_C,4
POT3_C,GT
VCP3_S1,PS,-
VCP3_S2,PS,-
VCP3_R3,PS,2

POT3_A,3
POT3_A,GT
VCP3_S2,PS,+
VCP3_R2,PS,2

#00052,4
VCP3_AVS1,PS,A
VCP3_AVS2,PS,A
VCP3_R1,PS,2
COMVDDINTRN#001F,PS,POT3V

AGND3,6
AGND3,GT
VCP3_R2,PS,1
VCP3_R3,PS,1
VCP3_R4,PS,1
VCP3_C1,PS,1
R3,PS,2

POT4_B,3
POT4_B,GT
VCP4_S1,PS,+
VCP4_R4,PS,2

POT4_C,4
POT4_C,GT
VCP4_S1,PS,-
VCP4_S2,PS,-
VCP4_R3,PS,2

POT4_A,3
POT4_A,GT
VCP4_S2,PS,+
VCP4_R2,PS,2

#00053,4
VCP4_AVS1,PS,A
VCP4_AVS2,PS,A
VCP4_R1,PS,2
COMVDDINTRN#001F,PS,POT4V

AGND4,6
AGND4,GT
VCP4_R2,PS,1
VCP4_R3,PS,1
VCP4_R4,PS,1
VCP4_C1,PS,1
R4,PS,2

POT5_B,3
POT5_B,GT
VCP5_S1,PS,+
VCP5_R4,PS,2

POT5_C,4
POT5_C,GT
VCP5_S1,PS,-
VCP5_S2,PS,-
VCP5_R3,PS,2

POT5_A,3
POT5_A,GT
VCP5_S2,PS,+
VCP5_R2,PS,2

#00054,4
VCP5_AVS1,PS,A
VCP5_AVS2,PS,A
VCP5_R1,PS,2
COMVDDINTRN#001F,PS,POT5V

AGND5,6
AGND5,GT
VCP5_R2,PS,1
VCP5_R3,PS,1
VCP5_R4,PS,1
VCP5_C1,PS,1
R16,PS,2

POT6_B,3
POT6_B,GT
VCP6_S1,PS,+
VCP6_R4,PS,2

POT6_C,4
POT6_C,GT
VCP6_S1,PS,-
VCP6_S2,PS,-
VCP6_R3,PS,2

POT6_A,3
POT6_A,GT
VCP6_S2,PS,+
VCP6_R2,PS,2

#00055,4
VCP6_AVS1,PS,A
VCP6_AVS2,PS,A
VCP6_R1,PS,2
COMVDDINTRN#001F,PS,POT6V

AGND6,6
AGND6,GT
VCP6_R2,PS,1
VCP6_R3,PS,1
VCP6_R4,PS,1
VCP6_C1,PS,1
R15,PS,2

POT7_B,3
POT7_B,GT
VCP7_S1,PS,+
VCP7_R4,PS,2

POT7_C,4
POT7_C,GT
VCP7_S1,PS,-
VCP7_S2,PS,-
VCP7_R3,PS,2

POT7_A,3
POT7_A,GT
VCP7_S2,PS,+
VCP7_R2,PS,2

#00056,4
VCP7_AVS1,PS,A
VCP7_AVS2,PS,A
VCP7_R1,PS,2
COMVDDINTRN#001F,PS,POT7V

AGND7,6
AGND7,GT
VCP7_R2,PS,1
VCP7_R3,PS,1
VCP7_R4,PS,1
VCP7_C1,PS,1
R14,PS,2

POT8_B,3
POT8_B,GT
VCP8_S1,PS,+
VCP8_R4,PS,2

POT8_C,4
POT8_C,GT
VCP8_S1,PS,-
VCP8_S2,PS,-
VCP8_R3,PS,2

POT8_A,3
POT8_A,GT
VCP8_S2,PS,+
VCP8_R2,PS,2

#00057,4
VCP8_AVS1,PS,A
VCP8_AVS2,PS,A
VCP8_R1,PS,2
COMVDDINTRN#001F,PS,POT8V

AGND8,6
AGND8,GT
VCP8_R2,PS,1
VCP8_R3,PS,1
VCP8_R4,PS,1
VCP8_C1,PS,1
R13,PS,2

POT9_B,3
POT9_B,GT
VCP9_S1,PS,+
VCP9_R4,PS,2

POT9_C,4
POT9_C,GT
VCP9_S1,PS,-
VCP9_S2,PS,-
VCP9_R3,PS,2

POT9_A,3
POT9_A,GT
VCP9_S2,PS,+
VCP9_R2,PS,2

#00058,4
VCP9_AVS1,PS,A
VCP9_AVS2,PS,A
VCP9_R1,PS,2
COMVDDINTRN#001F,PS,POT9V

AGND9,6
AGND9,GT
VCP9_R2,PS,1
VCP9_R3,PS,1
VCP9_R4,PS,1
VCP9_C1,PS,1
R5,PS,2

POT10_B,3
POT10_B,GT
VCP10_S1,PS,+
VCP10_R4,PS,2

POT10_C,4
POT10_C,GT
VCP10_S1,PS,-
VCP10_S2,PS,-
VCP10_R3,PS,2

POT10_A,3
POT10_A,GT
VCP10_S2,PS,+
VCP10_R2,PS,2

#00059,4
VCP10_AVS1,PS,A
VCP10_AVS2,PS,A
VCP10_R1,PS,2
COMVDDINTRN#001F,PS,POT10V

AGND10,6
AGND10,GT
VCP10_R2,PS,1
VCP10_R3,PS,1
VCP10_R4,PS,1
VCP10_C1,PS,1
R6,PS,2

POT11_B,3
POT11_B,GT
VCP11_S1,PS,+
VCP11_R4,PS,2

POT11_C,4
POT11_C,GT
VCP11_S1,PS,-
VCP11_S2,PS,-
VCP11_R3,PS,2

POT11_A,3
POT11_A,GT
VCP11_S2,PS,+
VCP11_R2,PS,2

#00060,4
VCP11_AVS1,PS,A
VCP11_AVS2,PS,A
VCP11_R1,PS,2
COMVDDINTRN#001F,PS,POT11V

AGND11,6
AGND11,GT
VCP11_R2,PS,1
VCP11_R3,PS,1
VCP11_R4,PS,1
VCP11_C1,PS,1
R7,PS,2

POT12_B,3
POT12_B,GT
VCP12_S1,PS,+
VCP12_R4,PS,2

POT12_C,4
POT12_C,GT
VCP12_S1,PS,-
VCP12_S2,PS,-
VCP12_R3,PS,2

POT12_A,3
POT12_A,GT
VCP12_S2,PS,+
VCP12_R2,PS,2

#00061,4
VCP12_AVS1,PS,A
VCP12_AVS2,PS,A
VCP12_R1,PS,2
COMVDDINTRN#001F,PS,POT12V

AGND12,6
AGND12,GT
VCP12_R2,PS,1
VCP12_R3,PS,1
VCP12_R4,PS,1
VCP12_C1,PS,1
R8,PS,2

POT13_B,3
POT13_B,GT
VCP13_S1,PS,+
VCP13_R4,PS,2

POT13_C,4
POT13_C,GT
VCP13_S1,PS,-
VCP13_S2,PS,-
VCP13_R3,PS,2

POT13_A,3
POT13_A,GT
VCP13_S2,PS,+
VCP13_R2,PS,2

#00062,4
VCP13_AVS1,PS,A
VCP13_AVS2,PS,A
VCP13_R1,PS,2
COMVDDINTRN#001F,PS,POT13V

AGND13,6
AGND13,GT
VCP13_R2,PS,1
VCP13_R3,PS,1
VCP13_R4,PS,1
VCP13_C1,PS,1
R9,PS,2

POT14_B,3
POT14_B,GT
VCP14_S1,PS,+
VCP14_R4,PS,2

POT14_C,4
POT14_C,GT
VCP14_S1,PS,-
VCP14_S2,PS,-
VCP14_R3,PS,2

POT14_A,3
POT14_A,GT
VCP14_S2,PS,+
VCP14_R2,PS,2

#00063,4
VCP14_AVS1,PS,A
VCP14_AVS2,PS,A
VCP14_R1,PS,2
COMVDDINTRN#001F,PS,POT14V

AGND14,6
AGND14,GT
VCP14_R2,PS,1
VCP14_R3,PS,1
VCP14_R4,PS,1
VCP14_C1,PS,1
R10,PS,2

POT15_B,3
POT15_B,GT
VCP15_S1,PS,+
VCP15_R4,PS,2

POT15_C,4
POT15_C,GT
VCP15_S1,PS,-
VCP15_S2,PS,-
VCP15_R3,PS,2

POT15_A,3
POT15_A,GT
VCP15_S2,PS,+
VCP15_R2,PS,2

#00064,4
VCP15_AVS1,PS,A
VCP15_AVS2,PS,A
VCP15_R1,PS,2
COMVDDINTRN#001F,PS,POT15V

AGND15,6
AGND15,GT
VCP15_R2,PS,1
VCP15_R3,PS,1
VCP15_R4,PS,1
VCP15_C1,PS,1
R11,PS,2

POT16_B,3
POT16_B,GT
VCP16_S1,PS,+
VCP16_R4,PS,2

POT16_C,4
POT16_C,GT
VCP16_S1,PS,-
VCP16_S2,PS,-
VCP16_R3,PS,2

POT16_A,3
POT16_A,GT
VCP16_S2,PS,+
VCP16_R2,PS,2

#00065,4
VCP16_AVS1,PS,A
VCP16_AVS2,PS,A
VCP16_R1,PS,2
COMVDDINTRN#001F,PS,POT16V

AGND16,6
AGND16,GT
VCP16_R2,PS,1
VCP16_R3,PS,1
VCP16_R4,PS,1
VCP16_C1,PS,1
R12,PS,2

GND,161
GND,PT
VCP16_C1,PS,2
VCP16_S1,PS,N
VCP16_AVS1,PS,-
VCP16_AVS2,PS,-
VCP16_AVS1,PS,B
VCP16_AVS2,PS,B
VCP16_R1,PS,1
VCP16_S2,PS,N
VCP15_C1,PS,2
VCP15_S1,PS,N
VCP15_AVS1,PS,-
VCP15_AVS2,PS,-
VCP15_AVS1,PS,B
VCP15_AVS2,PS,B
VCP15_R1,PS,1
VCP15_S2,PS,N
VCP14_C1,PS,2
VCP14_S1,PS,N
VCP14_AVS1,PS,-
VCP14_AVS2,PS,-
VCP14_AVS1,PS,B
VCP14_AVS2,PS,B
VCP14_R1,PS,1
VCP14_S2,PS,N
VCP13_C1,PS,2
VCP13_S1,PS,N
VCP13_AVS1,PS,-
VCP13_AVS2,PS,-
VCP13_AVS1,PS,B
VCP13_AVS2,PS,B
VCP13_R1,PS,1
VCP13_S2,PS,N
VCP12_C1,PS,2
VCP12_S1,PS,N
VCP12_AVS1,PS,-
VCP12_AVS2,PS,-
VCP12_AVS1,PS,B
VCP12_AVS2,PS,B
VCP12_R1,PS,1
VCP12_S2,PS,N
VCP11_C1,PS,2
VCP11_S1,PS,N
VCP11_AVS1,PS,-
VCP11_AVS2,PS,-
VCP11_AVS1,PS,B
VCP11_AVS2,PS,B
VCP11_R1,PS,1
VCP11_S2,PS,N
VCP10_C1,PS,2
VCP10_S1,PS,N
VCP10_AVS1,PS,-
VCP10_AVS2,PS,-
VCP10_AVS1,PS,B
VCP10_AVS2,PS,B
VCP10_R1,PS,1
VCP10_S2,PS,N
VCP9_C1,PS,2
VCP9_S1,PS,N
VCP9_AVS1,PS,-
VCP9_AVS2,PS,-
VCP9_AVS1,PS,B
VCP9_AVS2,PS,B
VCP9_R1,PS,1
VCP9_S2,PS,N
VCP8_C1,PS,2
VCP8_S1,PS,N
VCP8_AVS1,PS,-
VCP8_AVS2,PS,-
VCP8_AVS1,PS,B
VCP8_AVS2,PS,B
VCP8_R1,PS,1
VCP8_S2,PS,N
VCP7_C1,PS,2
VCP7_S1,PS,N
VCP7_AVS1,PS,-
VCP7_AVS2,PS,-
VCP7_AVS1,PS,B
VCP7_AVS2,PS,B
VCP7_R1,PS,1
VCP7_S2,PS,N
VCP6_C1,PS,2
VCP6_S1,PS,N
VCP6_AVS1,PS,-
VCP6_AVS2,PS,-
VCP6_AVS1,PS,B
VCP6_AVS2,PS,B
VCP6_R1,PS,1
VCP6_S2,PS,N
VCP5_C1,PS,2
VCP5_S1,PS,N
VCP5_AVS1,PS,-
VCP5_AVS2,PS,-
VCP5_AVS1,PS,B
VCP5_AVS2,PS,B
VCP5_R1,PS,1
VCP5_S2,PS,N
VCP4_C1,PS,2
VCP4_S1,PS,N
VCP4_AVS1,PS,-
VCP4_AVS2,PS,-
VCP4_AVS1,PS,B
VCP4_AVS2,PS,B
VCP4_R1,PS,1
VCP4_S2,PS,N
VCP3_C1,PS,2
VCP3_S1,PS,N
VCP3_AVS1,PS,-
VCP3_AVS2,PS,-
VCP3_AVS1,PS,B
VCP3_AVS2,PS,B
VCP3_R1,PS,1
VCP3_S2,PS,N
VCP2_C1,PS,2
VCP2_S1,PS,N
VCP2_AVS1,PS,-
VCP2_AVS2,PS,-
VCP2_AVS1,PS,B
VCP2_AVS2,PS,B
VCP2_R1,PS,1
VCP2_S2,PS,N
VCP1_C1,PS,2
VCP1_S1,PS,N
VCP1_AVS1,PS,-
VCP1_AVS2,PS,-
VCP1_AVS1,PS,B
VCP1_AVS2,PS,B
VCP1_R1,PS,1
VCP1_S2,PS,N
VBNK4_V4,PS,-
VBNK4_V3,PS,-
VBNK4_V2,PS,-
VBNK4_V1,PS,-
VBNK3_V4,PS,-
VBNK3_V3,PS,-
VBNK3_V2,PS,-
VBNK3_V1,PS,-
VBNK2_V4,PS,-
VBNK2_V3,PS,-
VBNK2_V2,PS,-
VBNK2_V1,PS,-
VBNK1_V4,PS,-
VBNK1_V3,PS,-
VBNK1_V2,PS,-
VBNK1_V1,PS,-
R16,PS,1
R15,PS,1
R14,PS,1
R13,PS,1
R12,PS,1
R11,PS,1
R10,PS,1
R9,PS,1
R8,PS,1
R7,PS,1
R6,PS,1
R5,PS,1
R4,PS,1
R3,PS,1
R2,PS,1
R1,PS,1

*GATES,0    

