LISA MODEL DESCRIPTION FORMAT 6.1
=================================
Design:   SLDVDD DECADE BOX MODEL
Doc. no.: 002
Revision: 003
Author:   SIMEON.DAVID.WEBBER.MCA
Created:  10/09/05
Modified: 01/01/07

*PROPERTIES,53   
16BUS=<16BUS>
APUDFREQ=<APUDFREQ>
BTE=16
BUTTONS=0
COMPVAL1=<POTVAL1>
COMPVAL2=<POTVAL2>
COMPVAL3=<POTVAL3>
COMPVAL4=<POTVAL4>
COMPVAL5=<POTVAL5>
COMPVAL6=<POTVAL6>
COMPVAL7=<POTVAL7>
COMPVAL8=<POTVAL8>
COMPVAL9=<POTVAL9>
COMPVAL10=<POTVAL10>
COMPVAL11=1000
COMPVAL12=1000
COMPVAL13=1000
COMPVAL14=1000
COMPVAL15=1000
COMPVAL16=1000
CRM=<CRM>
DEC=<DEC>
DECADE=<DECADE>
DECBD=<DECBD>
EEPROM=<EEPROM>
ENLCR=<ENLCR>
ENSAVED=<ENSAVED>
GR=1000T
HIDEOA=<HIDEOA>
LCR=<LCR>
LCRVHOA=<LCRVHOA>
MIDIPORTEN=<MIDIPORTEN>
POTVAL1=<POTVAL1>
POTVAL2=<POTVAL2>
POTVAL3=<POTVAL3>
POTVAL4=<POTVAL4>
POTVAL5=<POTVAL5>
POTVAL6=<POTVAL6>
POTVAL7=<POTVAL7>
POTVAL8=<POTVAL8>
POTVAL9=<POTVAL9>
POTVAL10=<POTVAL10>
POTVAL11=<POTVAL11>
PUVIEW=<PUVIEW>
RSPREAD=1000T
SDSSW=<SDSSW>
SHMEM=<SHMEM>
SLIDERS=1
SPRINGEN=<SPRINGEN>
SSPU=<SSPU>
SWITCHES=0
VDD=1
VDDHIDEOA=<VDDHIDEOA>

*MAPPINGS,4,STEP1
10 : AW_1VOLTS = 10,    REFV1 = 10
100 : AW_1VOLTS = 100,   REFV1 = 100
1000 : AW_1VOLTS = 1000,  REFV1 = 1000
10000 : AW_1VOLTS = 10000, REFV1 = 10000

*MAPPINGS,4,STEP2
10 : AW_2VOLTS = 10,    REFV2 = 10
100 : AW_2VOLTS = 100,   REFV2 = 100
1000 : AW_2VOLTS = 1000,  REFV2 = 1000
10000 : AW_2VOLTS = 10000, REFV2 = 10000

*MAPPINGS,4,STEP3
10 : AW_3VOLTS = 10,    REFV3 = 10
100 : AW_3VOLTS = 100,   REFV3 = 100
1000 : AW_3VOLTS = 1000,  REFV3 = 1000
10000 : AW_3VOLTS = 10000, REFV3 = 10000

*MAPPINGS,4,STEP4
10 : AW_4VOLTS = 10,    REFV4 = 10
100 : AW_4VOLTS = 100,   REFV4 = 100
1000 : AW_4VOLTS = 1000,  REFV4 = 1000
10000 : AW_4VOLTS = 10000, REFV4 = 10000

*MAPPINGS,4,STEP5
10 : AW_5VOLTS = 10,    REFV5 = 10
100 : AW_5VOLTS = 100,   REFV5 = 100
1000 : AW_5VOLTS = 1000,  REFV5 = 1000
10000 : AW_5VOLTS = 10000, REFV5 = 10000

*MAPPINGS,4,STEP6
10 : AW_6VOLTS = 10,    REFV6 = 10
100 : AW_6VOLTS = 100,   REFV6 = 100
1000 : AW_6VOLTS = 1000,  REFV6 = 1000
10000 : AW_6VOLTS = 10000, REFV6 = 10000

*MAPPINGS,4,STEP7
10 : AW_7VOLTS = 10,    REFV7 = 10
100 : AW_7VOLTS = 100,   REFV7 = 100
1000 : AW_7VOLTS = 1000,  REFV7 = 1000
10000 : AW_7VOLTS = 10000, REFV7 = 10000

*MAPPINGS,4,STEP8
10 : AW_8VOLTS = 10,    REFV8 = 10
100 : AW_8VOLTS = 100,   REFV8 = 100
1000 : AW_8VOLTS = 1000,  REFV8 = 1000
10000 : AW_8VOLTS = 10000, REFV8 = 10000

*MAPPINGS,4,STEP9
10 : AW_9VOLTS = 10,    REFV9 = 10
100 : AW_9VOLTS = 100,   REFV9 = 100
1000 : AW_9VOLTS = 1000,  REFV9 = 1000
10000 : AW_9VOLTS = 10000, REFV9 = 10000

*MAPPINGS,4,STEP10
10 : AW_10VOLTS = 10,    REFV10 = 10
100 : AW_10VOLTS = 100,   REFV10 = 100
1000 : AW_10VOLTS = 1000,  REFV10 = 1000
10000 : AW_10VOLTS = 10000, REFV10 = 10000

*MAPPINGS,4,STEP11
10 : AW_11VOLTS = 10,    REFV11 = 10
100 : AW_11VOLTS = 100,   REFV11 = 100
1000 : AW_11VOLTS = 1000,  REFV11 = 1000
10000 : AW_11VOLTS = 10000, REFV11 = 10000

*MODELDEFS,0    

*PARTLIST,57   
VBNK1_V1,VSOURCE,<REFV11>,PRIMITIVE=ANALOG
VBNK1_V2,VSOURCE,<REFV7>,PRIMITIVE=ANALOG
VBNK1_V3,VSOURCE,<REFV8>,PRIMITIVE=ANALOG
VBNK1_V4,VSOURCE,<REFV9>,PRIMITIVE=ANALOG
VBNK1_V5,VSOURCE,<REFV10>,PRIMITIVE=ANALOG
VBNK1_V6,VSOURCE,<REFV11>,PRIMITIVE=ANALOG
VBNK2_V1,VSOURCE,<REFV1>,PRIMITIVE=ANALOG
VBNK2_V2,VSOURCE,<REFV2>,PRIMITIVE=ANALOG
VBNK2_V3,VSOURCE,<REFV3>,PRIMITIVE=ANALOG
VBNK2_V4,VSOURCE,<REFV4>,PRIMITIVE=ANALOG
VBNK2_V5,VSOURCE,<REFV5>,PRIMITIVE=ANALOG
VCP1_R1,RESISTOR,1M,PRIMITIVE=ANALOGUE
VCP1_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP1_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP1_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL1>,VOFF=0,VON=<AW_1VOLTS>
VCP10_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP10_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP10_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP10_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL10>,VOFF=0,VON=<AW_10VOLTS>
VCP11_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP11_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP11_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP11_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL11>,VOFF=0,VON=<AW_11VOLTS>
VCP2_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP2_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP2_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP2_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL2>,VOFF=0,VON=<AW_2VOLTS>
VCP3_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP3_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP3_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP3_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL3>,VOFF=0,VON=<AW_3VOLTS>
VCP4_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP4_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP4_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP4_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL4>,VOFF=0,VON=<AW_4VOLTS>
VCP5_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP5_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP5_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP5_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL5>,VOFF=0,VON=<AW_5VOLTS>
VCP6_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP6_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP6_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP6_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL6>,VOFF=0,VON=<AW_6VOLTS>
VCP7_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP7_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP7_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP7_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL7>,VOFF=0,VON=<AW_7VOLTS>
VCP8_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP8_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP8_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP8_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL8>,VOFF=0,VON=<AW_8VOLTS>
VCP9_R1,RESISTOR,<RSPREAD>,PRIMITIVE=ANALOGUE
VCP9_R2,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP9_R3,RESISTOR,1000T,PRIMITIVE=ANALOGUE
VCP9_S1,VCR,VCR,PRIMITIVE=ANALOGUE,ROFF=1p,RON=<POTVAL9>,VOFF=0,VON=<AW_9VOLTS>
CLOCK#0002,DIGITAL!,,CLOCK=<APUDFREQ>,INIT=0,PRIMITIVE=DIGITAL
DECADE_BOX_INRN#0010,SLDVDD,,16BUS=<16BUS>,BTE=<BTE>,BTSWITCH=10n,BUTTONS=0,COMPVAL1=<COMPVAL1>,COMPVAL2=<COMPVAL2>,COMPVAL3=<COMPVAL3>,COMPVAL4=<COMPVAL4>,COMPVAL5=<COMPVAL5>,COMPVAL6=<COMPVAL6>,COMPVAL7=<COMPVAL7>,COMPVAL8=<COMPVAL8>,COMPVAL9=<COMPVAL9>,COMPVAL10=<COMPVAL10>,COMPVAL11=1000,COMPVAL12=1000,COMPVAL13=1000,COMPVAL14=1000,COMPVAL15=1000,COMPVAL16=1000,CRM=<CRM>,DEC=<DEC>,DECADE=<DECADE>,DECBD=<DECBD>,EEPROM=<EEPROM>,ENLCR=<ENLCR>,ENSAVED=<ENSAVED>,HIDEOA=<HIDEOA>,INITBTNS=00,INITSW=00,LCRV=<LCRV>,LCRVHOA=<LCRVHOA>,MIDIPORTEN=<MIDIPORTEN>,MODDLL=SLDVDD,PRIMITIVE=DIGITAL,ptCONV=1u,PUVIEW=<PUVIEW>,SDSSW=<SDSSW>,SHMEM=<SHMEM>,SLIDERS=1,SPRINGEN=<SPRINGEN>,SSPU=<SSPU>,STEPPING1=<REFV1>,STEPPING2=<REFV2>,STEPPING3=<REFV3>,STEPPING4=<REFV4>,STEPPING5=<REFV5>,STEPPING6=<REFV6>,STEPPING7=<REFV7>,STEPPING8=<REFV8>,STEPPING9=<REFV9>,STEPPING10=<REFV10>,STEPPING11=0,STEPPING12=0,STEPPING13=0,STEPPING14=0,STEPPING15=0,STEPPING16=0,STSWITCH=10n,SWITCHES=0,tsbCONV=2u,VDD=<VDD>,VDDHIDEOA=<VDDHIDEOA>,XPOTS=9

*NETLIST,80   
#00000,2
CLOCK#0002,OP,*
DECADE_BOX_INRN#0010,PS,PUDCLK

#00001,1
DECADE_BOX_INRN#0010,PS,SW_COM

#00002,1
DECADE_BOX_INRN#0010,PS,BTN_COM

#00003,1
DECADE_BOX_INRN#0010,IO,BTN1

#00004,1
DECADE_BOX_INRN#0010,IO,BTN2

#00005,1
DECADE_BOX_INRN#0010,IO,BTN3

#00006,1
DECADE_BOX_INRN#0010,IO,BTN4

#00007,1
DECADE_BOX_INRN#0010,IO,BTN5

#00008,1
DECADE_BOX_INRN#0010,IO,BTN6

#00009,1
DECADE_BOX_INRN#0010,IO,BTN7

#00010,1
DECADE_BOX_INRN#0010,IO,BTN8

#00011,1
DECADE_BOX_INRN#0010,IO,SW1

#00012,1
DECADE_BOX_INRN#0010,IO,SW2

#00013,1
DECADE_BOX_INRN#0010,IO,SW3

#00014,1
DECADE_BOX_INRN#0010,IO,SW4

#00015,1
DECADE_BOX_INRN#0010,IO,SW5

#00016,1
DECADE_BOX_INRN#0010,IO,SW6

#00017,1
DECADE_BOX_INRN#0010,IO,SW7

#00018,1
DECADE_BOX_INRN#0010,IO,SW8

SAVE,2
SAVE,IT
DECADE_BOX_INRN#0010,PS,SAVE

RELOAD,2
RELOAD,IT
DECADE_BOX_INRN#0010,PS,RELOAD

HOLDV,2
HOLDV,OT
DECADE_BOX_INRN#0010,OP,HOLDV

BDLOAD,2
BDLOAD,IT
DECADE_BOX_INRN#0010,PS,BDLOAD

RESET,2
RESET,IT
DECADE_BOX_INRN#0010,PS,RESET

EPLYRSEL,2
EPLYRSEL,IT
DECADE_BOX_INRN#0010,PS,EPLYRSEL

SEL1,2
SEL1,GT
DECADE_BOX_INRN#0010,PS,SEL1

SEL2,2
SEL2,GT
DECADE_BOX_INRN#0010,PS,SEL2

SEL3,2
SEL3,GT
DECADE_BOX_INRN#0010,PS,SEL3

SEL4,2
SEL4,GT
DECADE_BOX_INRN#0010,PS,SEL4

BD0,2
BD0,GT
DECADE_BOX_INRN#0010,PS,BD0

BD1,2
BD1,GT
DECADE_BOX_INRN#0010,PS,BD1

BD2,2
BD2,GT
DECADE_BOX_INRN#0010,PS,BD2

BD3,2
BD3,GT
DECADE_BOX_INRN#0010,PS,BD3

BD4,2
BD4,GT
DECADE_BOX_INRN#0010,PS,BD4

BD5,2
BD5,GT
DECADE_BOX_INRN#0010,PS,BD5

BD6,2
BD6,GT
DECADE_BOX_INRN#0010,PS,BD6

BD7,2
BD7,GT
DECADE_BOX_INRN#0010,PS,BD7

BD8,2
BD8,GT
DECADE_BOX_INRN#0010,PS,BD8

BD9,2
BD9,GT
DECADE_BOX_INRN#0010,PS,BD9

BD10,2
BD10,GT
DECADE_BOX_INRN#0010,PS,BD10

BD11,2
BD11,GT
DECADE_BOX_INRN#0010,PS,BD11

BD12,2
BD12,GT
DECADE_BOX_INRN#0010,PS,BD12

BD13,2
BD13,GT
DECADE_BOX_INRN#0010,PS,BD13

BD14,2
BD14,GT
DECADE_BOX_INRN#0010,PS,BD14

BD15,2
BD15,GT
DECADE_BOX_INRN#0010,PS,BD15

#00019,2
VBNK1_V1,PS,+
DECADE_BOX_INRN#0010,PS,POT6R

#00020,2
VBNK1_V2,PS,+
DECADE_BOX_INRN#0010,PS,POT7R

#00021,2
VBNK1_V3,PS,+
DECADE_BOX_INRN#0010,PS,POT8R

#00022,2
VBNK1_V4,PS,+
DECADE_BOX_INRN#0010,PS,POT9R

#00023,2
VBNK1_V5,PS,+
DECADE_BOX_INRN#0010,PS,POT10R

#00024,2
VBNK1_V6,PS,+
DECADE_BOX_INRN#0010,PS,POT11R

#00025,2
VBNK2_V1,PS,+
DECADE_BOX_INRN#0010,PS,POT1R

#00026,2
VBNK2_V2,PS,+
DECADE_BOX_INRN#0010,PS,POT2R

#00027,2
VBNK2_V3,PS,+
DECADE_BOX_INRN#0010,PS,POT3R

#00028,2
VBNK2_V4,PS,+
DECADE_BOX_INRN#0010,PS,POT4R

#00029,2
VBNK2_V5,PS,+
DECADE_BOX_INRN#0010,PS,POT5R

R2,3
R2,GT
VCP1_S1,PS,-
VCP1_R3,PS,1

#00030,3
VCP1_S1,PS,P
VCP1_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT1V

#00031,4
VCP2_S1,PS,-
VCP2_R3,PS,1
VCP1_S1,PS,+
VCP1_R2,PS,1

#00032,3
VCP2_S1,PS,P
VCP2_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT2V

#00033,4
VCP3_S1,PS,-
VCP3_R3,PS,1
VCP2_S1,PS,+
VCP2_R2,PS,1

#00034,3
VCP3_S1,PS,P
VCP3_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT3V

#00035,4
VCP4_S1,PS,-
VCP4_R3,PS,1
VCP3_S1,PS,+
VCP3_R2,PS,1

#00036,3
VCP4_S1,PS,P
VCP4_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT4V

#00037,4
VCP5_S1,PS,-
VCP5_R3,PS,1
VCP4_S1,PS,+
VCP4_R2,PS,1

#00038,3
VCP5_S1,PS,P
VCP5_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT5V

#00039,4
VCP6_S1,PS,-
VCP6_R3,PS,1
VCP5_S1,PS,+
VCP5_R2,PS,1

#00040,3
VCP6_S1,PS,P
VCP6_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT6V

#00041,4
VCP7_S1,PS,-
VCP7_R3,PS,1
VCP6_S1,PS,+
VCP6_R2,PS,1

#00042,3
VCP7_S1,PS,P
VCP7_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT7V

#00043,4
VCP8_S1,PS,-
VCP8_R3,PS,1
VCP7_S1,PS,+
VCP7_R2,PS,1

#00044,3
VCP8_S1,PS,P
VCP8_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT8V

#00045,4
VCP9_S1,PS,-
VCP9_R3,PS,1
VCP8_S1,PS,+
VCP8_R2,PS,1

#00046,3
VCP9_S1,PS,P
VCP9_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT9V

#00047,4
VCP10_S1,PS,-
VCP10_R3,PS,1
VCP9_S1,PS,+
VCP9_R2,PS,1

#00048,3
VCP10_S1,PS,P
VCP10_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT10V

R1,3
R1,GT
VCP11_S1,PS,+
VCP11_R2,PS,1

#00049,4
VCP11_S1,PS,-
VCP11_R3,PS,1
VCP10_S1,PS,+
VCP10_R2,PS,1

#00050,3
VCP11_S1,PS,P
VCP11_R1,PS,2
DECADE_BOX_INRN#0010,PS,POT11V

GND,57
GND,PT
AGND,GT
VCP11_S1,PS,N
VCP11_R1,PS,1
VCP11_R2,PS,2
VCP11_R3,PS,2
VCP10_S1,PS,N
VCP10_R1,PS,1
VCP10_R2,PS,2
VCP10_R3,PS,2
VCP9_S1,PS,N
VCP9_R1,PS,1
VCP9_R2,PS,2
VCP9_R3,PS,2
VCP8_S1,PS,N
VCP8_R1,PS,1
VCP8_R2,PS,2
VCP8_R3,PS,2
VCP7_S1,PS,N
VCP7_R1,PS,1
VCP7_R2,PS,2
VCP7_R3,PS,2
VCP6_S1,PS,N
VCP6_R1,PS,1
VCP6_R2,PS,2
VCP6_R3,PS,2
VCP5_S1,PS,N
VCP5_R1,PS,1
VCP5_R2,PS,2
VCP5_R3,PS,2
VCP4_S1,PS,N
VCP4_R1,PS,1
VCP4_R2,PS,2
VCP4_R3,PS,2
VCP3_S1,PS,N
VCP3_R1,PS,1
VCP3_R2,PS,2
VCP3_R3,PS,2
VCP2_S1,PS,N
VCP2_R1,PS,1
VCP2_R2,PS,2
VCP2_R3,PS,2
VCP1_S1,PS,N
VCP1_R1,PS,1
VCP1_R2,PS,2
VCP1_R3,PS,2
VBNK2_V5,PS,-
VBNK2_V4,PS,-
VBNK2_V3,PS,-
VBNK2_V2,PS,-
VBNK2_V1,PS,-
VBNK1_V5,PS,-
VBNK1_V4,PS,-
VBNK1_V3,PS,-
VBNK1_V2,PS,-
VBNK1_V1,PS,-
VBNK1_V6,PS,-

*GATES,0    

