LISA MODEL DESCRIPTION FORMAT 6.1
=================================
Design:   C:\Documents and Settings\ANYUSER\My Documents\ISIS PROJECTS\MIXED MODEL PROJECTS\COMVDD_ISIS_AUTOMATION\ISIS LIBRARY PARTS AND MODELS DESIGNS AND TEST DESIGNS\LISA MODELS DESIGNS AND SUBSHEETS\COMVDDSBO.DSN
Doc. no.: <NONE>
Revision: <NONE>
Author:   <NONE>
Created:  16/09/05
Modified: 30/07/06

*PROPERTIES,40   
APUDFREQ=<APUDFREQ>
BTE=<BTE>
BTNOFFRES=<BTNOFFRES>
BTNONRES=<BTNONRES>
BTNSWTIME=<BTNSWTIME>
BTSWITCH=<BTSWITCH>
BUTTONS=<BUTTONS>
CRM=<CRM>
DEC=<DEC>
DECADE=<DECADE>
DM=<DM>
DS=<DS>
ENSAVED=<ENSAVED>
GR=1T
HIDEOA=<HIDEOA>
INITBTNS=<INITBTNS>
INITSW=<INITSW>
PRERETRY=<PRERETRY>
PSDELAY=<PSDELAY>
PTM=<PTM>
PUVIEW=<PUVIEW>
RSPREAD=100k
SDSSW=<SDSSW>
SHMEM=<SHMEM>
SIMRETRY=<SIMRETRY>
SLIDERS=<SLIDERS>
SPRINGEN=0
SSDELAY=<SSDELAY>
SSPU=0
STSWITCH=<STSWITCH>
SWITCHES=<SWITCHES>
SWOFFRES=<SWOFFRES>
SWONRES=<SWONRES>
SWSWTIME=<SWSWTIME>
VD_BAUDRATE=<VD_BAUDRATE>
VD_DATABITS=<VD_DATABITS>
VD_PARITY=<VD_PARITY>
VD_PORT=<VD_PORT>
VD_STOPBITS=<VD_STOPBITS>
VDD=<VDD>

*MAPPINGS,1,APOTS
1 : XPOTS = 0,     ptCONV=1u , tsbCONV=2u

*MODELDEFS,0    

*PARTLIST,50   
DBNK1_SW1,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW2,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW3,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW4,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW5,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW6,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW7,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW8,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<BTNOFFRES>,RON=<BTNONRES>,TSWITCH=<BTNSWTIME>
DBNK1_SW9,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW10,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW11,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW12,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW13,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW14,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW15,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
DBNK1_SW16,DSWITCH,DSWITCH,PRIMITIVE=PASSIVE,ROFF=<SWOFFRES>,RON=<SWONRES>,TSWITCH=<SWSWTIME>
CLOCK#0002,DIGITAL!,,CLOCK=<APUDFREQ>,INIT=0,PRIMITIVE=DIGITAL
COMVDDINTRN#0001,COMVDD,,BTE=<BTE>,BTSWITCH=<BTSWITCH>,BUTTONS=<BUTTONS>,CRM=<CRM>,DEC=<DEC>,DECADE=<DECADE>,DM=<DM>,DS=<DS>,ENSAVED=<ENSAVED>,HIDEOA=<HIDEOA>,INITBTNS=<INITBTNS>,INITSW=<INITSW>,MODDLL=COMVDD,PRERETRY=<PRERETRY>,PRIMITIVE=DIGITAL,PSDELAY=<PSDELAY>,ptCONV=<ptCONV>,PTM=<PTM>,PUVIEW=<PUVIEW>,SDSSW=<SDSSW>,SHMEM=<SHMEM>,SIMRETRY=<SIMRETRY>,SLIDERS=<SLIDERS>,SPRINGEN=<SPRINGEN>,SSDELAY=<SSDELAY>,SSPU=<SSPU>,STSWITCH=<STSWITCH>,SWITCHES=<SWITCHES>,tsbCONV=<tsbCONV>,VD_BAUDRATE=<VD_BAUDRATE>,VD_DATABITS=<VD_DATABITS>,VD_PARITY=<VD_PARITY>,VD_PORT=<VD_PORT>,VD_STOPBITS=<VD_STOPBITS>,VDD=<VDD>,XPOTS=<XPOTS>
R1,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R2,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R3,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R4,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R5,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R6,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R7,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R8,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R9,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R10,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R11,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R12,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R13,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R14,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R15,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R16,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R17,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R18,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R19,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R20,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R21,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R22,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R23,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R24,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R25,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R26,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R27,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R28,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R29,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R30,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R31,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR
R32,RES,1T,PRIMITIVE=ANALOG,PRIMTYPE=RESISTOR

*NETLIST,80   
#00000,2
COMVDDINTRN#0001,PS,POT2V
R13,PS,2

#00001,2
COMVDDINTRN#0001,PS,POT4V
R9,PS,2

#00002,2
COMVDDINTRN#0001,PS,POT3V
R11,PS,2

#00003,2
COMVDDINTRN#0001,PS,POT9V
R18,PS,2

#00004,2
COMVDDINTRN#0001,PS,POT10V
R20,PS,2

#00005,2
COMVDDINTRN#0001,PS,POT12V
R24,PS,2

#00006,2
COMVDDINTRN#0001,PS,POT11V
R22,PS,2

#00007,2
COMVDDINTRN#0001,PS,POT2R
R14,PS,2

#00008,2
COMVDDINTRN#0001,PS,POT4R
R10,PS,2

#00009,2
COMVDDINTRN#0001,PS,POT3R
R12,PS,2

#00010,2
COMVDDINTRN#0001,PS,POT9R
R17,PS,2

#00011,2
COMVDDINTRN#0001,PS,POT10R
R19,PS,2

#00012,2
COMVDDINTRN#0001,PS,POT12R
R23,PS,2

#00013,2
COMVDDINTRN#0001,PS,POT11R
R21,PS,2

#00014,2
COMVDDINTRN#0001,PS,POT5V
R7,PS,2

#00015,2
COMVDDINTRN#0001,PS,POT6V
R5,PS,2

#00016,2
COMVDDINTRN#0001,PS,POT7V
R3,PS,2

#00017,2
COMVDDINTRN#0001,PS,POT5R
R8,PS,2

#00018,2
COMVDDINTRN#0001,PS,POT6R
R6,PS,2

#00019,2
COMVDDINTRN#0001,PS,POT7R
R4,PS,2

#00020,2
COMVDDINTRN#0001,PS,POT13V
R26,PS,2

#00021,2
COMVDDINTRN#0001,PS,POT14V
R28,PS,2

#00022,2
COMVDDINTRN#0001,PS,POT15V
R30,PS,2

#00023,2
COMVDDINTRN#0001,PS,POT13R
R25,PS,2

#00024,2
COMVDDINTRN#0001,PS,POT14R
R27,PS,2

#00025,2
COMVDDINTRN#0001,PS,POT15R
R29,PS,2

#00026,2
COMVDDINTRN#0001,PS,POT1V
R15,PS,2

#00027,2
COMVDDINTRN#0001,PS,POT1R
R16,PS,2

#00028,2
COMVDDINTRN#0001,PS,POT8V
R1,PS,2

#00029,2
COMVDDINTRN#0001,PS,POT8R
R2,PS,2

#00030,2
COMVDDINTRN#0001,PS,POT16V
R32,PS,2

#00031,2
COMVDDINTRN#0001,PS,POT16R
R31,PS,2

#00032,2
COMVDDINTRN#0001,PS,PUDCLK
CLOCK#0002,OP,*

#00033,1
COMVDDINTRN#0001,OP,HOLDV

BTND_COM,2
BTND_COM,IT
COMVDDINTRN#0001,PS,BTN_COM

RESET,2
RESET,IT
COMVDDINTRN#0001,PS,RESET

SWD_COM,2
SWD_COM,IT
COMVDDINTRN#0001,PS,SW_COM

SAVE,2
SAVE,IT
COMVDDINTRN#0001,PS,SAVE

RELOAD,2
RELOAD,IT
COMVDDINTRN#0001,PS,RELOAD

GND,33
GND,PT
R17,PS,1
R18,PS,1
R19,PS,1
R20,PS,1
R21,PS,1
R22,PS,1
R23,PS,1
R24,PS,1
R25,PS,1
R26,PS,1
R27,PS,1
R28,PS,1
R29,PS,1
R30,PS,1
R31,PS,1
R32,PS,1
R1,PS,1
R2,PS,1
R3,PS,1
R4,PS,1
R5,PS,1
R6,PS,1
R7,PS,1
R8,PS,1
R9,PS,1
R10,PS,1
R11,PS,1
R12,PS,1
R13,PS,1
R14,PS,1
R15,PS,1
R16,PS,1

BTN_COM1,3
BTN_COM1,GT
DBNK1_SW1,IO,A
DBNK1_SW2,IO,A

B1TN1,2
B1TN1,GT
DBNK1_SW1,IO,B

BTND1,3
BTND1,OT
DBNK1_SW1,IP,EN
COMVDDINTRN#0001,IO,BTN1

B1TN2,2
B1TN2,GT
DBNK1_SW2,IO,B

BTND2,3
BTND2,OT
DBNK1_SW2,IP,EN
COMVDDINTRN#0001,IO,BTN2

BTN_COM2,3
BTN_COM2,GT
DBNK1_SW3,IO,A
DBNK1_SW4,IO,A

B2TN3,2
B2TN3,GT
DBNK1_SW3,IO,B

BTND3,3
BTND3,OT
DBNK1_SW3,IP,EN
COMVDDINTRN#0001,IO,BTN3

B2TN4,2
B2TN4,GT
DBNK1_SW4,IO,B

BTND4,3
BTND4,OT
DBNK1_SW4,IP,EN
COMVDDINTRN#0001,IO,BTN4

BTN_COM3,3
BTN_COM3,GT
DBNK1_SW5,IO,A
DBNK1_SW6,IO,A

B3TN5,2
B3TN5,GT
DBNK1_SW5,IO,B

BTND5,3
BTND5,OT
DBNK1_SW5,IP,EN
COMVDDINTRN#0001,IO,BTN5

B3TN6,2
B3TN6,GT
DBNK1_SW6,IO,B

BTND6,3
BTND6,OT
DBNK1_SW6,IP,EN
COMVDDINTRN#0001,IO,BTN6

BTN_COM4,3
BTN_COM4,GT
DBNK1_SW7,IO,A
DBNK1_SW8,IO,A

B4TN7,2
B4TN7,GT
DBNK1_SW7,IO,B

BTND7,3
BTND7,OT
DBNK1_SW7,IP,EN
COMVDDINTRN#0001,IO,BTN7

B4TN8,2
B4TN8,GT
DBNK1_SW8,IO,B

BTND8,3
BTND8,OT
DBNK1_SW8,IP,EN
COMVDDINTRN#0001,IO,BTN8

SW_COM1,3
SW_COM1,GT
DBNK1_SW9,IO,A
DBNK1_SW10,IO,A

S1W1,2
S1W1,GT
DBNK1_SW9,IO,B

SWD1,3
SWD1,OT
DBNK1_SW9,IP,EN
COMVDDINTRN#0001,IO,SW1

S1W2,2
S1W2,GT
DBNK1_SW10,IO,B

SWD2,3
SWD2,OT
DBNK1_SW10,IP,EN
COMVDDINTRN#0001,IO,SW2

SW_COM2,3
SW_COM2,GT
DBNK1_SW11,IO,A
DBNK1_SW12,IO,A

S2W3,2
S2W3,GT
DBNK1_SW11,IO,B

SWD3,3
SWD3,OT
DBNK1_SW11,IP,EN
COMVDDINTRN#0001,IO,SW3

S2W4,2
S2W4,GT
DBNK1_SW12,IO,B

SWD4,3
SWD4,OT
DBNK1_SW12,IP,EN
COMVDDINTRN#0001,IO,SW4

SW_COM3,3
SW_COM3,GT
DBNK1_SW13,IO,A
DBNK1_SW14,IO,A

S3W5,2
S3W5,GT
DBNK1_SW13,IO,B

SWD5,3
SWD5,OT
DBNK1_SW13,IP,EN
COMVDDINTRN#0001,IO,SW5

S3W6,2
S3W6,GT
DBNK1_SW14,IO,B

SWD6,3
SWD6,OT
DBNK1_SW14,IP,EN
COMVDDINTRN#0001,IO,SW6

SW_COM4,3
SW_COM4,GT
DBNK1_SW15,IO,A
DBNK1_SW16,IO,A

S4W7,2
S4W7,GT
DBNK1_SW15,IO,B

SWD7,3
SWD7,OT
DBNK1_SW15,IP,EN
COMVDDINTRN#0001,IO,SW7

S4W8,2
S4W8,GT
DBNK1_SW16,IO,B

SWD8,3
SWD8,OT
DBNK1_SW16,IP,EN
COMVDDINTRN#0001,IO,SW8

*GATES,0    

